EESchema-DOCLIB  Version 2.0
#
$CMP CRYSTAL-16MHZPTH-HC49US
D 16MHz Crystal <a href="http://www.digikey.com/product-search/en?keywords=535-9122-1-ND">Digikey Example</a> <ul><li>Frequency: 16MHz</li><li>Frequency Stability: &plusmn;50ppm</li><li>Frequency Tolerance: &plusmn;20ppm</li><li>Load Capacitance: 18pF</li></ul> <b>SparkFun Products:</b><ul><li><a href= https://www.sparkfun.com/products/12640 >Pro Micro -5V/16MHz</a></li><li><a href= https://www.sparkfun.com/products/10097 >SparkFun Serial Enabled LCD Kit</a></li></ul> 
K PROD_ID:XTAL-08181
$ENDCMP
#
$CMP CRYSTAL-16MHZSMD-5X3.2
D 16MHz Crystal <a href="http://www.digikey.com/product-search/en?keywords=535-9122-1-ND">Digikey Example</a> <ul><li>Frequency: 16MHz</li><li>Frequency Stability: &plusmn;50ppm</li><li>Frequency Tolerance: &plusmn;20ppm</li><li>Load Capacitance: 18pF</li></ul> <b>SparkFun Products:</b><ul><li><a href= https://www.sparkfun.com/products/12640 >Pro Micro -5V/16MHz</a></li><li><a href= https://www.sparkfun.com/products/10097 >SparkFun Serial Enabled LCD Kit</a></li></ul> 
K PROD_ID:XTAL-08218
$ENDCMP
#
$CMP CRYSTAL-26MHZSMD-3.2X2.5
D 26MHz Crystal w/ Ground Pin <a href="http://www.digikey.com/product-detail/en/epson/TSX-3225%2026.0000MF09Z-AC3/SER3627CT-ND/1802878">Digikey Example</a> <ul><li>Frequency: 26MHz</li><li>Frequency Stability: &plusmn;9ppm</li><li>Frequency Tolerance: &plusmn;10ppm</li><li>Load Capacitance: 9pF</li></ul> <b>SparkFun Products:</b><ul><li><a href= https://www.sparkfun.com/products/13907 >SparkFun ESP32 Thing</a></li><li><a href= https://www.sparkfun.com/products/13711 >SparkFun ESP8266 Thing Dev Board</a></li></ul> 
K PROD_ID:XTAL-12454
$ENDCMP
#
$CMP CRYSTAL-32.768KHZPTH-2X6
D 32.768kHz Crystal <ul><li>Frequency: 32.768kHz</li><li>Frequency Stability: &plusmn;20ppm</li><li>Load Capacitance: 12.5pF (PTH-2X6 & SMD-3.2X1.5), 6pF (SMD-2X6)</li></ul> <b>SparkFun Products:</b><ul><li><a href= https://www.sparkfun.com/products/11734 >SparkFun BigTime Watch Kit</a></li><li><a href= https://www.sparkfun.com/products/13990 >SparkFun nRF52832 Breakout</a></li><li><a href= https://www.sparkfun.com/products/12708 >SparkFun Real Time Clock Module</a></li></ul> 
K PROD_ID:XTAL-10112
$ENDCMP
#
$CMP CRYSTAL-32.768KHZPTH-2X6-KIT
D 32.768kHz Crystal <ul><li>Frequency: 32.768kHz</li><li>Frequency Stability: &plusmn;20ppm</li><li>Load Capacitance: 12.5pF (PTH-2X6 & SMD-3.2X1.5), 6pF (SMD-2X6)</li></ul> <b>SparkFun Products:</b><ul><li><a href= https://www.sparkfun.com/products/11734 >SparkFun BigTime Watch Kit</a></li><li><a href= https://www.sparkfun.com/products/13990 >SparkFun nRF52832 Breakout</a></li><li><a href= https://www.sparkfun.com/products/12708 >SparkFun Real Time Clock Module</a></li></ul> 
K PROD_ID:XTAL-10112
$ENDCMP
#
$CMP CRYSTAL-32.768KHZSMD-2X6
D 32.768kHz Crystal <ul><li>Frequency: 32.768kHz</li><li>Frequency Stability: &plusmn;20ppm</li><li>Load Capacitance: 12.5pF (PTH-2X6 & SMD-3.2X1.5), 6pF (SMD-2X6)</li></ul> <b>SparkFun Products:</b><ul><li><a href= https://www.sparkfun.com/products/11734 >SparkFun BigTime Watch Kit</a></li><li><a href= https://www.sparkfun.com/products/13990 >SparkFun nRF52832 Breakout</a></li><li><a href= https://www.sparkfun.com/products/12708 >SparkFun Real Time Clock Module</a></li></ul> 
K PROD_ID:XTAL-07894
$ENDCMP
#
$CMP CRYSTAL-32.768KHZSMD-3.2X1.5
D 32.768kHz Crystal <ul><li>Frequency: 32.768kHz</li><li>Frequency Stability: &plusmn;20ppm</li><li>Load Capacitance: 12.5pF (PTH-2X6 & SMD-3.2X1.5), 6pF (SMD-2X6)</li></ul> <b>SparkFun Products:</b><ul><li><a href= https://www.sparkfun.com/products/11734 >SparkFun BigTime Watch Kit</a></li><li><a href= https://www.sparkfun.com/products/13990 >SparkFun nRF52832 Breakout</a></li><li><a href= https://www.sparkfun.com/products/12708 >SparkFun Real Time Clock Module</a></li></ul> 
K PROD_ID:XTAL-13062
$ENDCMP
#
$CMP CRYSTAL-32.768KHZSMD-MC146
D 32.768kHz Crystal <ul><li>Frequency: 32.768kHz</li><li>Frequency Stability: &plusmn;20ppm</li><li>Load Capacitance: 12.5pF (PTH-2X6 & SMD-3.2X1.5), 6pF (SMD-2X6)</li></ul> <b>SparkFun Products:</b><ul><li><a href= https://www.sparkfun.com/products/11734 >SparkFun BigTime Watch Kit</a></li><li><a href= https://www.sparkfun.com/products/13990 >SparkFun nRF52832 Breakout</a></li><li><a href= https://www.sparkfun.com/products/12708 >SparkFun Real Time Clock Module</a></li></ul> 
K PROD_ID:XTAL-09342
$ENDCMP
#
$CMP CRYSTAL-32MHZ-SMD-2.0X1.6MM
D 32MHz Crystal <a href="http://www.digikey.com/product-detail/en/murata-electronics-north-america/XRCGB32M000F2P00R0/490-9769-1-ND/4952013">Digikey Example</a><ul><li>Frequency: 32MHz</li><li>Frequency Stability:  20ppm</li><li>Frequency Tolerance:  20ppm</li><li>Load Capacitance: 6pF</li></ul> SparkFun Products <ul><li><a href= https://www.sparkfun.com/products/13990 >SparkFun nRF52832 Breakout</a></li></ul> 
K PROD_ID:XTAL-13459
$ENDCMP
#
$CMP CRYSTAL-8MHZSMD-5X3.2
D 8MHz Crystal <a href="http://www.futureelectronics.com/en/technologies/electromechanical/timing-devices/crystals/Pages/6008189-ABM3B-8.000MHZ-B2-T.aspx?IM=0">Datasheet Example</a> <ul><li>Frequency: 8MHz</li><li>Frequency Tolerance: &plusmn;20ppm</li><li>Load Capacitance: 18pF</li></ul> <b>SparkFun Products:</b><ul><li><a href= https://www.sparkfun.com/products/12587 >Pro Micro -3.3V/8MHz</a></li><li><a href= https://www.sparkfun.com/products/13660 >WAV Trigger</a></li></ul> 
K PROD_ID:XTAL-09431
$ENDCMP
#
$CMP CRYSTAL-8MHZSMD-HC49UP
D 8MHz Crystal <a href="http://www.futureelectronics.com/en/technologies/electromechanical/timing-devices/crystals/Pages/6008189-ABM3B-8.000MHZ-B2-T.aspx?IM=0">Datasheet Example</a> <ul><li>Frequency: 8MHz</li><li>Frequency Tolerance: &plusmn;20ppm</li><li>Load Capacitance: 18pF</li></ul> <b>SparkFun Products:</b><ul><li><a href= https://www.sparkfun.com/products/12587 >Pro Micro -3.3V/8MHz</a></li><li><a href= https://www.sparkfun.com/products/13660 >WAV Trigger</a></li></ul> 
K PROD_ID:XTAL-11706
$ENDCMP
#
$CMP CRYSTAL-GROUNDEDSMD-3.2X2.5
D Crystals w/ Ground Pin (Generic) These are <b>passive</b> quartz crystals, which can be used as a clock source for a microcontroller. Crystal's are usually two-terminal devices. A third terminal may be optionally connected to ground, as recommended by the manufaturer. 
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP CRYSTAL-GROUNDEDSMD-5X3.2
D Crystals w/ Ground Pin (Generic) These are <b>passive</b> quartz crystals, which can be used as a clock source for a microcontroller. Crystal's are usually two-terminal devices. A third terminal may be optionally connected to ground, as recommended by the manufaturer. 
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP CRYSTALPTH-2X6
D Crystals (Generic) These are <b>passive</b> quartz crystals, which can be used as a clock source for a microcontroller. Crystal's are two-terminal devices. They require external "load" capacitors to generate an oscillating signal. 
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP CRYSTALPTH-2X6-KIT
D Crystals (Generic) These are <b>passive</b> quartz crystals, which can be used as a clock source for a microcontroller. Crystal's are two-terminal devices. They require external "load" capacitors to generate an oscillating signal. 
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP CRYSTALPTH-3X8
D Crystals (Generic) These are <b>passive</b> quartz crystals, which can be used as a clock source for a microcontroller. Crystal's are two-terminal devices. They require external "load" capacitors to generate an oscillating signal. 
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP CRYSTALPTH-HC49US
D Crystals (Generic) These are <b>passive</b> quartz crystals, which can be used as a clock source for a microcontroller. Crystal's are two-terminal devices. They require external "load" capacitors to generate an oscillating signal. 
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP CRYSTALPTH-HC49UV
D Crystals (Generic) These are <b>passive</b> quartz crystals, which can be used as a clock source for a microcontroller. Crystal's are two-terminal devices. They require external "load" capacitors to generate an oscillating signal. 
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP CRYSTALSMD-2X6
D Crystals (Generic) These are <b>passive</b> quartz crystals, which can be used as a clock source for a microcontroller. Crystal's are two-terminal devices. They require external "load" capacitors to generate an oscillating signal. 
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP CRYSTALSMD-3.2X1.5
D Crystals (Generic) These are <b>passive</b> quartz crystals, which can be used as a clock source for a microcontroller. Crystal's are two-terminal devices. They require external "load" capacitors to generate an oscillating signal. 
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP CRYSTALSMD-3.2X2.5
D Crystals (Generic) These are <b>passive</b> quartz crystals, which can be used as a clock source for a microcontroller. Crystal's are two-terminal devices. They require external "load" capacitors to generate an oscillating signal. 
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP CRYSTALSMD-5X3.2-2PAD
D Crystals (Generic) These are <b>passive</b> quartz crystals, which can be used as a clock source for a microcontroller. Crystal's are two-terminal devices. They require external "load" capacitors to generate an oscillating signal. 
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP CRYSTALSMD-5X3.2-4PAD
D Crystals (Generic) These are <b>passive</b> quartz crystals, which can be used as a clock source for a microcontroller. Crystal's are two-terminal devices. They require external "load" capacitors to generate an oscillating signal. 
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP CRYSTALSMD-HC49UP
D Crystals (Generic) These are <b>passive</b> quartz crystals, which can be used as a clock source for a microcontroller. Crystal's are two-terminal devices. They require external "load" capacitors to generate an oscillating signal. 
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP CRYSTALSMD-MC146
D Crystals (Generic) These are <b>passive</b> quartz crystals, which can be used as a clock source for a microcontroller. Crystal's are two-terminal devices. They require external "load" capacitors to generate an oscillating signal. 
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP DS1077U
D Maxim DS1077 - I2C Real-time clock (RTC) The   DS1077   is   a   dual-output,   programmable,   fixed-frequency   oscillator   requiring   no   external   components for operation. The DS1077 can be used as a processor-controlled frequency synthesizer or as  a  standalone  oscillator. The  DS1077  features  a  2-wire  serial  interface  that  allows  in-circuit  on-the-fly  programming  of the  programmable  prescalers  (P0  &  P1)  and  divider  (N)  with  the  desired  values  being  stored  in  NV  (EEPROM)   memory. SparkFun Products:<ul><li><a href="https://www.sparkfun.com/products/retired/99">Real Time Clock Module</a> (BOB-00099)</li></ul><a href="http://datasheets.maximintegrated.com/en/ds/DS1077.pdf">Datasheet</a> 
K PROD_ID:IC-09075
$ENDCMP
#
$CMP DS1307Z
D Maxim DS1307 - I2C Real-time clock (RTC) The  DS1307  serial  real-time  clock  (RTC)  is  a  low-power, full binary-coded decimal (BCD) clock/calendar plus  56  bytes  of  NV  SRAM.  Address  and  data  are transferred  serially  through  an  I2C,  bidirectional  bus. The clock/calendar provides seconds, minutes, hours, day,  date,  month,  and  year  information. SparkFun Products:<ul><li><a href="https://www.sparkfun.com/products/12708">Real Time Clock Module</a> (BOB-12708)</li></ul><a href="https://cdn.sparkfun.com/datasheets/BreakoutBoards/DS1307.pdf">Datasheet</a> 
K PROD_ID:IC-08138
$ENDCMP
#
$CMP DS3231M
D DS3231M Real Time Clock Accuracy +/-5ppm.  Battery Backup.  2.3V to 5.5V. <a href="https://cdn.sparkfun.com/datasheets/Dev/Beagle/DS3231M.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/12773">CryptoCape</a> (DEV-12773)</li><li><a href="https://www.sparkfun.com/products/13183">SparkFun CryptoShield</a> (DEV-13183)</li></ul>
K PROD_ID:IC-11985
$ENDCMP
#
$CMP DS3234
D Maxim DS3234 - Extremely Accurate SPI RTC The  DS3234  is  a  low-cost,  extremely  accurate  SPI   bus real-time clock (RTC) with an integrated temperature-compensated crystal oscillator (TCXO) and crystal. SparkFun Products:<ul><li><a href="https://www.sparkfun.com/products/10079">Real Time Clock - DS3234</a> (COM-10079)</li><li><a href="https://www.sparkfun.com/products/10160">SparkFun DeadOn RTC Breakout</a> (BOB-10160)</a></li></ul><a href="https://www.sparkfun.com/datasheets/BreakoutBoards/DS3234.pdf">Datasheet</a> 
K PROD_ID:IC-10016
$ENDCMP
#
$CMP OSCILLATOR-16MHZSMD-7X5-4PAD
D 16 MHz 7x5mm Oscllator <ul><li>Frequency: 16MHz</li><li>Frequency Stability: &plusmn;50ppm</li><li>Operating Voltage: 3.3V</li></ul> <a href="http://www.futureelectronics.com/en/technologies/electromechanical/timing-devices/oscillators/Pages/9907304-FXO-HC735-16.aspx?IM=0"> Datasheet Example</a> <ul><li><a href= https://www.sparkfun.com/products/11420 >SparkFun MiniGen</a></li></ul> 
K PROD_ID:XTAL-11225
$ENDCMP
#
$CMP OSCILLATOR-33MHZ
D 33 MHz 5x3.2mm Oscllator <ul><li>Standard 5.0mm x 3.2m 4-pad SMD package</li><li>Frequency: 33MHz</li><li>Frequency Stability: &plusmn;50ppm</li><li>Operating Voltage: 3.3V</li></ul> <a href="http://www.ctscorp.com/wp-content/uploads/2015/11/008-0250-0.pdf">Example datasheet</a>  SparkFun Products: <ul><li><a href= https://www.sparkfun.com/products/12773 >SparkFun CryptoCape</a></li></ul> 
K PROD_ID:XTAL-11986
$ENDCMP
#
$CMP OSCILLATORSMD-5X3
D Oscillators (Generic) These are <b>active</b> oscillators, which require a power source to generate their clock output. Most oscillators are configured to generate a set frequency (e.g. 16MHz). They have four pins: power, ground, output, and an enable input. 
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP OSCILLATORSMD-7X5-4PAD
D Oscillators (Generic) These are <b>active</b> oscillators, which require a power source to generate their clock output. Most oscillators are configured to generate a set frequency (e.g. 16MHz). They have four pins: power, ground, output, and an enable input. 
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP OSCILLATORSMD-7X5-6PAD
D Oscillators (Generic) These are <b>active</b> oscillators, which require a power source to generate their clock output. Most oscillators are configured to generate a set frequency (e.g. 16MHz). They have four pins: power, ground, output, and an enable input. 
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP RESONATOR-16MHZSMD_3.2X1.3
D 16MHz Resonator <a href="http://www.digikey.com/product-detail/en/murata-electronics-north-america/CSTCE16M0V53-R0/490-1198-1-ND/584635">Digikey Example</a> <ul><li>Frequency: 16MHz</li><li>Frequency Stability: &plusmn;0.3%</li><li>Frequency Tolerance: &plusmn;0.5%</li><li>Capacitance: 15pF</li></ul> SparkFun Products <ul><li><a href= https://www.sparkfun.com/products/13712 >SparkFun OpenLog</a></li><li><a href= https://www.sparkfun.com/products/12923 >SparkFun MicroView - OLED Arduino Module</a></li></ul> 
K PROD_ID:XTAL-08900
$ENDCMP
#
$CMP RESONATOR-4MHZSMD-4.5X2
D 4MHz Resonator <a href="http://www.digikey.com/product-search/en?keywords=490-1200-1-ND">Digikey Example</a> <ul><li>Frequency: 4MHz</li><li>Frequency Stability: &plusmn;0.2%</li><li>Frequency Tolerance: &plusmn;0.5%</li><li>Capacitance: 15pF</li></ul> SparkFun Products <ul><li><a href= https://www.sparkfun.com/products/13333 >SparkFun BadgerHack</a></li></ul> 
K PROD_ID:XTAL-12492
$ENDCMP
#
$CMP RESONATOR-8MHZSMD_3.2X1.3
D 8MHz Resonator <a href="http://www.digikey.com/product-detail/en/murata-electronics-north-america/CSTCE10M0G55-R0/490-1196-1-ND/584633">Digikey Example</a> <ul><li>Frequency: 8MHz</li><li>Frequency Stability: &plusmn;0.2%</li><li>Frequency Tolerance: &plusmn;0.5%</li><li>Capacitance: 33pF</li></ul> SparkFun Products <ul><li><a href= https://www.sparkfun.com/products/11114 >Arduino Pro Mini 328- 3.3V/8MHz</a></li><li><a href= https://www.sparkfun.com/products/12651 >SparkFun Digital Sandbox</a></li></ul> 
K PROD_ID:XTAL-08895
$ENDCMP
#
$CMP RESONATORPTH-7.6X3.8
D Resonators (Generic) Ceramic resonators are clock-generating components, often used to control timing in microcontrollers. They usually have 3 pins: two pins for oscillation, and one pin for ground. Compared to crystals, resonators have worse tolerance, but are usually much cheaper. Plus, they have built-in load capacitors! These devices are used on boards like the <a href="https://www.sparkfun.com/products/11114">Arduino Pro 8MHz</a> and <a href="https://www.sparkfun.com/products/11113">Arduino Pro 16MHz</a>. 
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP RESONATORSMD-3.2X1.3
D Resonators (Generic) Ceramic resonators are clock-generating components, often used to control timing in microcontrollers. They usually have 3 pins: two pins for oscillation, and one pin for ground. Compared to crystals, resonators have worse tolerance, but are usually much cheaper. Plus, they have built-in load capacitors! These devices are used on boards like the <a href="https://www.sparkfun.com/products/11114">Arduino Pro 8MHz</a> and <a href="https://www.sparkfun.com/products/11113">Arduino Pro 16MHz</a>. 
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP RESONATORSMD-4.5X2.0
D Resonators (Generic) Ceramic resonators are clock-generating components, often used to control timing in microcontrollers. They usually have 3 pins: two pins for oscillation, and one pin for ground. Compared to crystals, resonators have worse tolerance, but are usually much cheaper. Plus, they have built-in load capacitors! These devices are used on boards like the <a href="https://www.sparkfun.com/products/11114">Arduino Pro 8MHz</a> and <a href="https://www.sparkfun.com/products/11113">Arduino Pro 16MHz</a>. 
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP RESONATORSMD-7.4X3.4
D Resonators (Generic) Ceramic resonators are clock-generating components, often used to control timing in microcontrollers. They usually have 3 pins: two pins for oscillation, and one pin for ground. Compared to crystals, resonators have worse tolerance, but are usually much cheaper. Plus, they have built-in load capacitors! These devices are used on boards like the <a href="https://www.sparkfun.com/products/11114">Arduino Pro 8MHz</a> and <a href="https://www.sparkfun.com/products/11113">Arduino Pro 16MHz</a>. 
K PROD_ID:XXX-00000
$ENDCMP
#
#End Doc Library
