(module STANDOFF-ELECTRICAL (layer F.Cu) (tedit 200000)
  (descr "STANDOFF (#4 SCREW) - W/ ELECTRICAL CONNECTION")
  (tags "STANDOFF (#4 SCREW) - W/ ELECTRICAL CONNECTION")
  (attr virtual)
  (fp_text reference >NAME (at 0 -3.81) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 0 3.81) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (pad P1 thru_hole circle (at 0 0) (size 6.35 6.35) (drill 3.19786) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
