(module 1X12_LONGPADS (layer F.Cu) (tedit 5963D9D3)
  (descr "PLATED THROUGH HOLE -12 PIN LONG PADS")
  (tags "PLATED THROUGH HOLE -12 PIN LONG PADS")
  (attr virtual)
  (fp_text reference >NAME (at 0 -2.54) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 0 2.667) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_line (start -1.27 -0.635) (end -1.27 0.635) (layer F.SilkS) (width 0.2032))
  (fp_line (start 29.21 -0.635) (end 29.21 0.635) (layer F.SilkS) (width 0.2032))
  (pad 1 thru_hole oval (at 0 0 180) (size 1.8796 3.7592) (drill 1.1176) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 2 thru_hole oval (at 2.54 0 180) (size 1.8796 3.7592) (drill 1.1176) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 3 thru_hole oval (at 5.08 0 180) (size 1.8796 3.7592) (drill 1.1176) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 4 thru_hole oval (at 7.62 0 180) (size 1.8796 3.7592) (drill 1.1176) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 5 thru_hole oval (at 10.16 0 180) (size 1.8796 3.7592) (drill 1.1176) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 6 thru_hole oval (at 12.7 0 180) (size 1.8796 3.7592) (drill 1.1176) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 7 thru_hole oval (at 15.24 0 180) (size 1.8796 3.7592) (drill 1.1176) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 8 thru_hole oval (at 17.78 0 180) (size 1.8796 3.7592) (drill 1.1176) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 9 thru_hole oval (at 20.32 0 180) (size 1.8796 3.7592) (drill 1.1176) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 10 thru_hole oval (at 22.86 0 180) (size 1.8796 3.7592) (drill 1.1176) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 11 thru_hole oval (at 25.4 0 180) (size 1.8796 3.7592) (drill 1.1176) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 12 thru_hole oval (at 27.94 0 180) (size 1.8796 3.7592) (drill 1.1176) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
