(module SPARKFUN_PRO_MICRO (layer F.Cu) (tedit 200000)
  (descr "SPARKFUN PRO MICO FOOTPRINT (WITH USB CONNECTOR)")
  (tags "SPARKFUN PRO MICO FOOTPRINT (WITH USB CONNECTOR)")
  (attr virtual)
  (fp_text reference >NAME (at 0 -15.24) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 0 15.24) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_line (start -8.89 -16.51) (end -8.89 16.51) (layer Dwgs.User) (width 0.127))
  (fp_line (start -8.89 16.51) (end 8.89 16.51) (layer Dwgs.User) (width 0.127))
  (fp_line (start 8.89 16.51) (end 8.89 -16.51) (layer Dwgs.User) (width 0.127))
  (fp_line (start 8.89 -16.51) (end -8.89 -16.51) (layer Dwgs.User) (width 0.127))
  (fp_line (start -3.81 -16.51) (end -3.81 -17.78) (layer Dwgs.User) (width 0.127))
  (fp_line (start -3.81 -17.78) (end 3.81 -17.78) (layer Dwgs.User) (width 0.127))
  (fp_line (start 3.81 -17.78) (end 3.81 -16.51) (layer Dwgs.User) (width 0.127))
  (fp_text user USB (at -0.0508 -16.9164) (layer Dwgs.User)
    (effects (font (size 0.8128 0.8128) (thickness 0.1524)))
  )
  (pad 1 thru_hole circle (at -7.62 -12.7) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 2 thru_hole circle (at -7.62 -10.16) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 3 thru_hole circle (at -7.62 -7.62) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 4 thru_hole circle (at -7.62 -5.08) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 5 thru_hole circle (at -7.62 -2.54) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 6 thru_hole circle (at -7.62 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 7 thru_hole circle (at -7.62 2.54) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 8 thru_hole circle (at -7.62 5.08) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 9 thru_hole circle (at -7.62 7.62) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 10 thru_hole circle (at -7.62 10.16) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 11 thru_hole circle (at -7.62 12.7) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 12 thru_hole circle (at -7.62 15.24) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 13 thru_hole circle (at 7.62 15.24) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 14 thru_hole circle (at 7.62 12.7) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 15 thru_hole circle (at 7.62 10.16) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 16 thru_hole circle (at 7.62 7.62) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 17 thru_hole circle (at 7.62 5.08) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 18 thru_hole circle (at 7.62 2.54) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 19 thru_hole circle (at 7.62 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 20 thru_hole circle (at 7.62 -2.54) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 21 thru_hole circle (at 7.62 -5.08) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 22 thru_hole circle (at 7.62 -7.62) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 23 thru_hole circle (at 7.62 -10.16) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 24 thru_hole circle (at 7.62 -12.7) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
