(module 2X5-RAF (layer F.Cu) (tedit 5963E316)
  (descr "PLATED THROUGH HOLE - 2X5 RIGHT ANGLE FEMALE HEADER")
  (tags "PLATED THROUGH HOLE - 2X5 RIGHT ANGLE FEMALE HEADER")
  (attr virtual)
  (fp_text reference >NAME (at 3.81 -6.858) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 3.81 6.985) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_line (start -2.54 -5.715) (end -2.54 -4.445) (layer F.SilkS) (width 0.2032))
  (fp_line (start 2.69748 -6.2992) (end 11.19886 -6.2992) (layer F.SilkS) (width 0.2032))
  (fp_line (start 11.19886 -6.2992) (end 11.19886 6.2992) (layer F.SilkS) (width 0.2032))
  (fp_line (start 11.19886 6.2992) (end 2.69748 6.2992) (layer F.SilkS) (width 0.2032))
  (fp_line (start 2.69748 6.2992) (end 2.69748 -6.2992) (layer F.SilkS) (width 0.2032))
  (fp_line (start 8.19912 -6.9977) (end 8.19912 6.89864) (layer Dwgs.User) (width 0.127))
  (fp_line (start -2.54 -5.715) (end -2.54 -4.445) (layer F.SilkS) (width 0.2032))
  (pad 1 thru_hole circle (at -1.27 -5.08) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 2 thru_hole circle (at 1.27 -5.08) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 3 thru_hole circle (at -1.27 -2.54) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 4 thru_hole circle (at 1.27 -2.54) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 5 thru_hole circle (at -1.27 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 6 thru_hole circle (at 1.27 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 7 thru_hole circle (at -1.27 2.54) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 8 thru_hole circle (at 1.27 2.54) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 9 thru_hole circle (at -1.27 5.08) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 10 thru_hole circle (at 1.27 5.08) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
