(module REED_SWITCH_PLASTIC (layer F.Cu) (tedit 200000)
  (descr "REED SWITCH - INSULATED CASE - PTH")
  (tags "REED SWITCH - INSULATED CASE - PTH")
  (attr virtual)
  (fp_text reference >NAME (at 0 -2.286) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 0 2.286) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_line (start -7.49808 1.64846) (end 7.49808 1.64846) (layer F.SilkS) (width 0.2032))
  (fp_line (start -7.49808 1.64846) (end -7.49808 0) (layer F.SilkS) (width 0.2032))
  (fp_line (start -7.49808 0) (end -7.49808 -1.64846) (layer F.SilkS) (width 0.2032))
  (fp_line (start -7.49808 -1.64846) (end 7.49808 -1.64846) (layer F.SilkS) (width 0.2032))
  (fp_line (start 7.49808 -1.64846) (end 7.49808 0) (layer F.SilkS) (width 0.2032))
  (fp_line (start 7.49808 0) (end 7.49808 1.64846) (layer F.SilkS) (width 0.2032))
  (fp_line (start -7.49808 0) (end -7.71906 0) (layer F.SilkS) (width 0.2032))
  (fp_line (start 7.49808 0) (end 7.71906 0) (layer F.SilkS) (width 0.2032))
  (pad P$1 thru_hole circle (at -8.89 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad P$2 thru_hole circle (at 8.89 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
