(module CPOL-RADIAL-2.5MM-5MM-KIT (layer F.Cu) (tedit 200000)
  (descr "2.5 MM SPACED PTHS WITH TOP COPPER MASKED")
  (tags "2.5 MM SPACED PTHS WITH TOP COPPER MASKED")
  (attr virtual)
  (fp_text reference >NAME (at 0 -3.048) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 0 3.175) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_line (start 0.28448 0.9652) (end 2.21488 0.9652) (layer F.SilkS) (width 0.06604))
  (fp_line (start 2.21488 0.9652) (end 2.21488 -0.9652) (layer F.SilkS) (width 0.06604))
  (fp_line (start 0.28448 -0.9652) (end 2.21488 -0.9652) (layer F.SilkS) (width 0.06604))
  (fp_line (start 0.28448 0.9652) (end 0.28448 -0.9652) (layer F.SilkS) (width 0.06604))
  (fp_line (start -0.74168 -1.397) (end -1.75768 -1.397) (layer F.SilkS) (width 0.2032))
  (fp_line (start 1.75768 -1.397) (end 0.74168 -1.397) (layer F.SilkS) (width 0.2032))
  (fp_line (start 1.24968 -1.905) (end 1.24968 -0.889) (layer F.SilkS) (width 0.2032))
  (fp_circle (center 0 0) (end 0 -2.49936) (layer F.SilkS) (width 0.2032))
  (fp_circle (center -1.24968 0) (end -1.24968 -0.3556) (layer F.SilkS) (width 0))
  (fp_circle (center -1.24968 0) (end -1.24968 -0.9652) (layer F.SilkS) (width 0))
  (fp_circle (center 1.24968 0) (end 1.24968 -0.3556) (layer F.SilkS) (width 0))
  (pad 1 thru_hole rect (at 1.24968 0) (size 1.651 1.651) (drill 0.6985) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 2 thru_hole circle (at -1.24968 0) (size 1.651 1.651) (drill 0.6985) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
