(module TACTILE_SWITCH_SMD_6.2MM_TALL (layer F.Cu) (tedit 200000)
  (descr "MOMENTARY SWITCH (PUSHBUTTON) - SPST - SMD, 6.2MM SQUARE")
  (tags "MOMENTARY SWITCH (PUSHBUTTON) - SPST - SMD, 6.2MM SQUARE")
  (attr smd)
  (fp_text reference >NAME (at 0 -3.556) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 0 3.683) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_line (start -2.99974 2.99974) (end 2.99974 2.99974) (layer F.SilkS) (width 0.2032))
  (fp_line (start 2.99974 2.99974) (end 2.99974 -2.99974) (layer F.SilkS) (width 0.2032))
  (fp_line (start 2.99974 -2.99974) (end -2.99974 -2.99974) (layer F.SilkS) (width 0.2032))
  (fp_line (start -2.99974 -2.99974) (end -2.99974 2.99974) (layer F.SilkS) (width 0.2032))
  (fp_circle (center 0 0) (end 0 -1.74752) (layer F.SilkS) (width 0.2032))
  (pad A1 smd rect (at -3.97256 2.2479 90) (size 1.29794 1.5494) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad A2 smd rect (at 3.97256 2.2479 90) (size 1.29794 1.5494) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad B1 smd rect (at -3.97256 -2.2479 90) (size 1.29794 1.5494) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad B2 smd rect (at 3.97256 -2.2479 90) (size 1.29794 1.5494) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
)
