(module STEREOJACK2.5MM_SPECIAL_POGOPINS (layer F.Cu) (tedit 200000)
  (descr "2.5MM STEREO AUDIO JACK - PTH POGO PIN COMPATIBLE")
  (tags "2.5MM STEREO AUDIO JACK - PTH POGO PIN COMPATIBLE")
  (attr virtual)
  (fp_text reference "" (at 0 0) (layer F.SilkS)
    (effects (font (thickness 0.15)))
  )
  (fp_text value "" (at 0 0) (layer F.SilkS)
    (effects (font (thickness 0.15)))
  )
  (fp_line (start 4.59994 -2.49936) (end -3.29946 -2.49936) (layer F.SilkS) (width 0.127))
  (fp_line (start -3.29946 -2.49936) (end -3.29946 -1.69926) (layer F.SilkS) (width 0.127))
  (fp_line (start -3.29946 -1.69926) (end -3.29946 1.89992) (layer F.SilkS) (width 0.127))
  (fp_line (start -3.29946 1.89992) (end -3.29946 2.59842) (layer F.SilkS) (width 0.127))
  (fp_line (start -3.29946 2.59842) (end 4.59994 2.59842) (layer F.SilkS) (width 0.127))
  (fp_line (start 4.59994 2.59842) (end 4.59994 1.4986) (layer F.SilkS) (width 0.127))
  (fp_line (start 4.59994 -1.4986) (end 4.59994 -2.49936) (layer F.SilkS) (width 0.127))
  (fp_line (start -3.29946 -1.69926) (end -6.2992 -1.69926) (layer F.SilkS) (width 0.127))
  (fp_line (start -6.2992 -1.69926) (end -6.2992 1.89992) (layer F.SilkS) (width 0.127))
  (fp_line (start -6.2992 1.89992) (end -3.29946 1.89992) (layer F.SilkS) (width 0.127))
  (pad RING thru_hole rect (at 2.49936 1.84912) (size 1.9304 0) (drill 1.1176) (layers *.Cu *.Mask) (solder_mask_margin 0.1016))
  (pad RING thru_hole rect (at 2.49936 -1.84912) (size 1.9304 0) (drill 1.1176) (layers *.Cu *.Mask) (solder_mask_margin 0.1016))
  (pad SHIE thru_hole rect (at -2.39776 0) (size 1.9304 0) (drill 1.1176) (layers *.Cu *.Mask) (solder_mask_margin 0.1016))
  (pad TIP thru_hole rect (at 4.49834 0) (size 1.9304 0) (drill 1.1176) (layers *.Cu *.Mask) (solder_mask_margin 0.1016))
  (pad "" np_thru_hole circle (at 0 0) (size 1.19888 1.19888) (drill 1.19888) (layers *.Cu *.Mask) (solder_mask_margin 0.1016))
)
