(module 2X20_SHROUDED_SMT (layer F.Cu) (tedit 200000)
  (descr "SURFACE MOUNT - 2X20 SHROUDED HEADER")
  (tags "SURFACE MOUNT - 2X20 SHROUDED HEADER")
  (attr smd)
  (fp_text reference >NAME (at 6.35 -24.13 90) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at -6.604 -24.13 90) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_line (start -5.94868 -24.765) (end -5.94868 -23.495) (layer F.SilkS) (width 0.2032))
  (fp_line (start 4.49834 -29.14904) (end 4.49834 29.14904) (layer F.SilkS) (width 0.2032))
  (fp_line (start -4.49834 29.14904) (end -4.49834 -29.14904) (layer F.SilkS) (width 0.2032))
  (fp_line (start -4.49834 -29.14904) (end 4.39928 -29.14904) (layer F.SilkS) (width 0.2032))
  (fp_line (start 4.49834 29.14904) (end -4.49834 29.14904) (layer F.SilkS) (width 0.2032))
  (fp_line (start -3.39852 -28.04922) (end 3.39852 -28.04922) (layer Dwgs.User) (width 0.2032))
  (fp_line (start 3.39852 -28.04922) (end 3.39852 28.04922) (layer Dwgs.User) (width 0.2032))
  (fp_line (start -3.39852 28.04922) (end 3.39852 28.04922) (layer Dwgs.User) (width 0.2032))
  (fp_line (start -3.39852 -28.04922) (end -3.39852 -2.19964) (layer Dwgs.User) (width 0.2032))
  (fp_line (start -3.39852 28.04922) (end -3.39852 2.19964) (layer Dwgs.User) (width 0.2032))
  (fp_line (start -4.49834 -2.19964) (end -2.99974 -2.19964) (layer F.SilkS) (width 0.2032))
  (fp_line (start -2.99974 2.19964) (end -4.49834 2.19964) (layer F.SilkS) (width 0.2032))
  (fp_line (start -2.99974 -2.19964) (end -2.99974 2.19964) (layer F.SilkS) (width 0.2032))
  (fp_line (start -5.98678 -24.765) (end -5.98678 -23.495) (layer F.SilkS) (width 0.2032))
  (pad 1 smd rect (at -3.5687 -24.13) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 2 smd rect (at 3.5687 -24.13) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 3 smd rect (at -3.5687 -21.59) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 4 smd rect (at 3.5687 -21.59) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 5 smd rect (at -3.5687 -19.05) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 6 smd rect (at 3.5687 -19.05) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 7 smd rect (at -3.5687 -16.51) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 8 smd rect (at 3.5687 -16.51) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 9 smd rect (at -3.5687 -13.97) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 10 smd rect (at 3.5687 -13.97) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 11 smd rect (at -3.5687 -11.43) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 12 smd rect (at 3.5687 -11.43) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 13 smd rect (at -3.5687 -8.89) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 14 smd rect (at 3.5687 -8.89) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 15 smd rect (at -3.5687 -6.35) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 16 smd rect (at 3.5687 -6.35) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 17 smd rect (at -3.5687 -3.81) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 18 smd rect (at 3.5687 -3.81) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 19 smd rect (at -3.5687 -1.27) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 20 smd rect (at 3.5687 -1.27) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 21 smd rect (at -3.5687 1.27) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 22 smd rect (at 3.5687 1.27) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 23 smd rect (at -3.5687 3.81) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 24 smd rect (at 3.5687 3.81) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 25 smd rect (at -3.5687 6.35) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 26 smd rect (at 3.5687 6.35) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 27 smd rect (at -3.5687 8.89) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 28 smd rect (at 3.5687 8.89) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 29 smd rect (at -3.5687 11.43) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 30 smd rect (at 3.5687 11.43) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 31 smd rect (at -3.5687 13.97) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 32 smd rect (at 3.5687 13.97) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 33 smd rect (at -3.5687 16.51) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 34 smd rect (at 3.5687 16.51) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 35 smd rect (at -3.5687 19.05) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 36 smd rect (at 3.5687 19.05) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 37 smd rect (at -3.5687 21.59) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 38 smd rect (at 3.5687 21.59) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 39 smd rect (at -3.5687 24.13) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 40 smd rect (at 3.5687 24.13) (size 4.1402 0.9906) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
)
