(module 1X17_NO_SILK_KIT (layer F.Cu) (tedit 200000)
  (descr "PLATED THROUGH HOLE -17 PIN NO SILK KIT")
  (tags "PLATED THROUGH HOLE -17 PIN NO SILK KIT")
  (attr virtual)
  (fp_text reference >NAME (at 0 -1.7018) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 0 1.7272) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_circle (center 0 0) (end 0 -0.508) (layer F.SilkS) (width 0))
  (fp_circle (center 0 0) (end 0 -0.9398) (layer F.SilkS) (width 0))
  (fp_circle (center 2.54 0) (end 2.54 -0.508) (layer F.SilkS) (width 0))
  (fp_circle (center 2.54 0) (end 2.54 -0.9398) (layer F.SilkS) (width 0))
  (fp_circle (center 5.08 0) (end 5.08 -0.508) (layer F.SilkS) (width 0))
  (fp_circle (center 5.08 0) (end 5.08 -0.9398) (layer F.SilkS) (width 0))
  (fp_circle (center 7.62 0) (end 7.62 -0.508) (layer F.SilkS) (width 0))
  (fp_circle (center 7.62 0) (end 7.62 -0.9398) (layer F.SilkS) (width 0))
  (fp_circle (center 10.16 0) (end 10.16 -0.508) (layer F.SilkS) (width 0))
  (fp_circle (center 10.16 0) (end 10.16 -0.9398) (layer F.SilkS) (width 0))
  (fp_circle (center 12.7 0) (end 12.7 -0.508) (layer F.SilkS) (width 0))
  (fp_circle (center 12.7 0) (end 12.7 -0.9398) (layer F.SilkS) (width 0))
  (fp_circle (center 15.24 0) (end 15.24 -0.508) (layer F.SilkS) (width 0))
  (fp_circle (center 15.24 0) (end 15.24 -0.9398) (layer F.SilkS) (width 0))
  (fp_circle (center 17.78 0) (end 17.78 -0.508) (layer F.SilkS) (width 0))
  (fp_circle (center 17.78 0) (end 17.78 -0.9398) (layer F.SilkS) (width 0))
  (fp_circle (center 20.32 0) (end 20.32 -0.508) (layer F.SilkS) (width 0))
  (fp_circle (center 20.32 0) (end 20.32 -0.9398) (layer F.SilkS) (width 0))
  (fp_circle (center 22.86 0) (end 22.86 -0.508) (layer F.SilkS) (width 0))
  (fp_circle (center 22.86 0) (end 22.86 -0.9398) (layer F.SilkS) (width 0))
  (fp_circle (center 25.4 0) (end 25.4 -0.508) (layer F.SilkS) (width 0))
  (fp_circle (center 25.4 0) (end 25.4 -0.9398) (layer F.SilkS) (width 0))
  (fp_circle (center 27.94 0) (end 27.94 -0.508) (layer F.SilkS) (width 0))
  (fp_circle (center 27.94 0) (end 27.94 -0.9398) (layer F.SilkS) (width 0))
  (fp_circle (center 30.48 0) (end 30.48 -0.508) (layer F.SilkS) (width 0))
  (fp_circle (center 30.48 0) (end 30.48 -0.9398) (layer F.SilkS) (width 0))
  (fp_circle (center 33.02 0) (end 33.02 -0.508) (layer F.SilkS) (width 0))
  (fp_circle (center 33.02 0) (end 33.02 -0.9398) (layer F.SilkS) (width 0))
  (fp_circle (center 35.56 0) (end 35.56 -0.508) (layer F.SilkS) (width 0))
  (fp_circle (center 35.56 0) (end 35.56 -0.9398) (layer F.SilkS) (width 0))
  (fp_circle (center 38.1 0) (end 38.1 -0.508) (layer F.SilkS) (width 0))
  (fp_circle (center 38.1 0) (end 38.1 -0.9398) (layer F.SilkS) (width 0))
  (fp_circle (center 40.64 0) (end 40.64 -0.508) (layer F.SilkS) (width 0))
  (fp_circle (center 40.64 0) (end 40.64 -0.9398) (layer F.SilkS) (width 0))
  (pad 1 thru_hole circle (at 0 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 2 thru_hole circle (at 2.54 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 3 thru_hole circle (at 5.08 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 4 thru_hole circle (at 7.62 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 5 thru_hole circle (at 10.16 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 6 thru_hole circle (at 12.7 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 7 thru_hole circle (at 15.24 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 8 thru_hole circle (at 17.78 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 9 thru_hole circle (at 20.32 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 10 thru_hole circle (at 22.86 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 11 thru_hole circle (at 25.4 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 12 thru_hole circle (at 27.94 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 13 thru_hole circle (at 30.48 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 14 thru_hole circle (at 33.02 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 15 thru_hole circle (at 35.56 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 16 thru_hole circle (at 38.1 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 17 thru_hole circle (at 40.64 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
