(module 2X3_TEST_POINTS (layer F.Cu) (tedit 200000)
  (descr "PLATED THROUGH HOLE - 2X3 TEST POINT HEADER")
  (tags "PLATED THROUGH HOLE - 2X3 TEST POINT HEADER")
  (attr virtual)
  (fp_text reference >NAME (at -2.54 -2.413) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at -2.54 2.794) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_line (start -2.8956 2.0574) (end -2.20726 2.0574) (layer F.SilkS) (width 0.2032))
  (fp_line (start -2.18186 2.0574) (end -2.8702 2.0574) (layer F.SilkS) (width 0.2032))
  (fp_circle (center -2.54 -1.27) (end -2.54 -1.8796) (layer F.SilkS) (width 0))
  (fp_circle (center 0 -1.27) (end 0 -1.8796) (layer F.SilkS) (width 0))
  (fp_circle (center 2.54 -1.27) (end 2.54 -1.8796) (layer F.SilkS) (width 0))
  (fp_circle (center -2.54 1.27) (end -2.54 0.6604) (layer F.SilkS) (width 0))
  (fp_circle (center 0 1.27) (end 0 0.6604) (layer F.SilkS) (width 0))
  (fp_circle (center 2.54 1.27) (end 2.54 0.6604) (layer F.SilkS) (width 0))
  (pad 1 thru_hole circle (at -2.54 1.27) (size 1.016 1.016) (drill 0.508) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 2 thru_hole circle (at -2.54 -1.27) (size 1.016 1.016) (drill 0.508) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 3 thru_hole circle (at 0 1.27) (size 1.016 1.016) (drill 0.508) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 4 thru_hole circle (at 0 -1.27) (size 1.016 1.016) (drill 0.508) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 5 thru_hole circle (at 2.54 1.27) (size 1.016 1.016) (drill 0.508) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 6 thru_hole circle (at 2.54 -1.27) (size 1.016 1.016) (drill 0.508) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
