(module 1X02_LONGPADS (layer F.Cu) (tedit 200000)
  (descr "PLATED THROUGH HOLE - LONG PADS WITHOUT SILK OUTLINE")
  (tags "PLATED THROUGH HOLE - LONG PADS WITHOUT SILK OUTLINE")
  (attr virtual)
  (fp_text reference >NAME (at 0 -2.54) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 0 2.54) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (pad 1 thru_hole oval (at 0 0 180) (size 1.8796 3.7592) (drill 1.1176) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 2 thru_hole oval (at 2.54 0 180) (size 1.8796 3.7592) (drill 1.1176) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
