(module TRIMPOT-SMD-3MM-CLOSED (layer F.Cu) (tedit 200000)
  (descr "TRIMPOT - SMD, 3MM SQUARE, CLOSED-FRAME")
  (tags "TRIMPOT - SMD, 3MM SQUARE, CLOSED-FRAME")
  (attr smd)
  (fp_text reference >NAME (at -2.159 0 90) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 2.286 0 90) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_line (start -0.99822 -1.59766) (end -1.59766 -1.59766) (layer F.SilkS) (width 0.2032))
  (fp_line (start -1.59766 -1.59766) (end -1.59766 1.59766) (layer F.SilkS) (width 0.2032))
  (fp_line (start 0.99822 -1.59766) (end 1.59766 -1.59766) (layer F.SilkS) (width 0.2032))
  (fp_line (start 1.59766 -1.59766) (end 1.59766 1.59766) (layer F.SilkS) (width 0.2032))
  (pad 1 smd rect (at -0.84836 1.64846) (size 0.99822 0.89916) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 2 smd rect (at 0 -1.64846) (size 1.09982 0.89916) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 3 smd rect (at 0.84836 1.64846) (size 0.99822 0.89916) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
)
