(module TP_15TH (layer F.Cu) (tedit 5963ECE7)
  (descr "ELECTRICALLY CONDUCTIVE VIA 0.015\" DRILL")
  (tags "ELECTRICALLY CONDUCTIVE VIA 0.015\" DRILL")
  (attr virtual)
  (fp_text reference Ref** (at 0 -0.889) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value Val** (at 0 0.889) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_circle (center 0 0) (end 0 -0.381) (layer F.SilkS) (width 0))
  (pad P$1 thru_hole circle (at 0 0) (size 0.6096 0.6096) (drill 0.381) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
