(module 1X08_FEMALE_LOCK (layer F.Cu) (tedit 5963D6AE)
  (descr "PLATED THROUGH HOLE -8 PIN LOCKING FEMALE HEADERS")
  (tags "PLATED THROUGH HOLE -8 PIN LOCKING FEMALE HEADERS")
  (attr virtual)
  (fp_text reference >NAME (at 0 -1.905) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 0 1.905) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_line (start -1.27 -1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.2032))
  (fp_line (start -1.27 -1.27) (end 19.05 -1.27) (layer F.SilkS) (width 0.2032))
  (fp_line (start 19.05 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.2032))
  (fp_line (start 19.05 -1.27) (end 19.05 1.27) (layer F.SilkS) (width 0.2032))
  (pad 1 thru_hole circle (at 0 -0.2286) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 2 thru_hole circle (at 2.54 0.2286) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 3 thru_hole circle (at 5.08 -0.2286) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 4 thru_hole circle (at 7.62 0.2286) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 5 thru_hole circle (at 10.16 -0.2286) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 6 thru_hole circle (at 12.7 0.2286) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 7 thru_hole circle (at 15.24 -0.2286) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 8 thru_hole circle (at 17.78 0.2286) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
