(module RockerSwitch_RA (layer F.Cu) (tedit 596A717E)
  (fp_text reference REF** (at 0 19.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value RockerSwitch_RA (at 0.5 -1) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user "pcb edge" (at 0 1) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 9.5 0) (end 9.5 2) (layer F.SilkS) (width 0.15))
  (fp_line (start -9.5 0) (end -9.5 2) (layer F.SilkS) (width 0.15))
  (fp_line (start 9.5 0) (end -9.5 0) (layer F.SilkS) (width 0.15))
  (pad 1 thru_hole circle (at 0 16) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 7 16) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 0 13) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 7 13) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask))
)
