(module 2X5-PTH-1.27MM (layer F.Cu) (tedit 200000)
  (descr "PLATED THROUGH HOLE - 2X5 ARM CORTEX DEBUG CONNECTOR (10-PIN)")
  (tags "PLATED THROUGH HOLE - 2X5 ARM CORTEX DEBUG CONNECTOR (10-PIN)")
  (attr virtual)
  (fp_text reference >NAME (at 0 -1.905) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 0 1.905) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_line (start -3.40106 1.01854) (end -3.40106 0.25654) (layer F.SilkS) (width 0.254))
  (fp_line (start 3.175 -1.7145) (end -3.175 -1.7145) (layer Dwgs.User) (width 0.127))
  (fp_line (start -3.175 -1.7145) (end -3.175 1.7145) (layer Dwgs.User) (width 0.127))
  (fp_line (start -3.175 1.7145) (end 3.175 1.7145) (layer Dwgs.User) (width 0.127))
  (fp_line (start 3.175 1.7145) (end 3.175 -1.7145) (layer Dwgs.User) (width 0.127))
  (pad 1 thru_hole circle (at -2.54 0.635) (size 0.99822 0.99822) (drill 0.508) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 2 thru_hole circle (at -2.54 -0.635) (size 0.99822 0.99822) (drill 0.508) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 3 thru_hole circle (at -1.27 0.635) (size 0.99822 0.99822) (drill 0.508) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 4 thru_hole circle (at -1.27 -0.635) (size 0.99822 0.99822) (drill 0.508) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 5 thru_hole circle (at 0 0.635) (size 0.99822 0.99822) (drill 0.508) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 6 thru_hole circle (at 0 -0.635) (size 0.99822 0.99822) (drill 0.508) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 7 thru_hole circle (at 1.27 0.635) (size 0.99822 0.99822) (drill 0.508) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 8 thru_hole circle (at 1.27 -0.635) (size 0.99822 0.99822) (drill 0.508) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 9 thru_hole circle (at 2.54 0.635) (size 0.99822 0.99822) (drill 0.508) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 10 thru_hole circle (at 2.54 -0.635) (size 0.99822 0.99822) (drill 0.508) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
