(module JST-5-PTH (layer F.Cu) (tedit 200000)
  (descr "JST 5 PIN RIGHT ANGLE PLATED THROUGH HOLE")
  (tags "JST 5 PIN RIGHT ANGLE PLATED THROUGH HOLE")
  (attr virtual)
  (fp_text reference >NAME (at -6.477 0 90) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 6.604 0 90) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_line (start -5.94868 1.59766) (end -5.94868 -5.99948) (layer F.SilkS) (width 0.2032))
  (fp_line (start -5.94868 -5.99948) (end 5.94868 -5.99948) (layer F.SilkS) (width 0.2032))
  (fp_line (start 5.94868 -5.99948) (end 5.94868 1.59766) (layer F.SilkS) (width 0.2032))
  (fp_line (start -5.94868 1.59766) (end -5.29844 1.59766) (layer F.SilkS) (width 0.2032))
  (fp_line (start 5.94868 1.59766) (end 5.29844 1.59766) (layer F.SilkS) (width 0.2032))
  (fp_line (start -5.29844 1.59766) (end -5.29844 0) (layer F.SilkS) (width 0.2032))
  (fp_line (start 5.29844 1.59766) (end 5.29844 0) (layer F.SilkS) (width 0.2032))
  (pad 1 thru_hole circle (at -3.99796 0) (size 1.59766 1.59766) (drill 0.6985) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 2 thru_hole circle (at -1.99898 0) (size 1.59766 1.59766) (drill 0.6985) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 3 thru_hole circle (at 0 0) (size 1.59766 1.59766) (drill 0.6985) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 4 thru_hole circle (at 1.99898 0) (size 1.59766 1.59766) (drill 0.6985) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 5 thru_hole circle (at 3.99796 0) (size 1.59766 1.59766) (drill 0.6985) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
