(module MOLEX_1X6_RA_LOCK (layer F.Cu) (tedit 200000)
  (descr "MOLEX 6-PIN PLATED THROUGH-HOLE RIGHT ANGLE LOCKING FOOTPRINT")
  (tags "MOLEX 6-PIN PLATED THROUGH-HOLE RIGHT ANGLE LOCKING FOOTPRINT")
  (attr virtual)
  (fp_text reference >NAME (at -0.635 -5.08 90) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 13.335 -5.08 90) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_line (start -1.27 -0.635) (end -1.27 -3.175) (layer F.SilkS) (width 0.127))
  (fp_line (start 13.97 -0.635) (end 13.97 -3.175) (layer F.SilkS) (width 0.127))
  (fp_line (start 13.97 -0.635) (end -1.27 -0.635) (layer F.SilkS) (width 0.127))
  (fp_line (start 13.97 -3.175) (end 12.7 -3.175) (layer F.SilkS) (width 0.127))
  (fp_line (start 12.7 -3.175) (end 0 -3.175) (layer F.SilkS) (width 0.127))
  (fp_line (start 0 -3.175) (end -1.27 -3.175) (layer F.SilkS) (width 0.127))
  (fp_line (start 0 -3.175) (end 0 -7.62) (layer F.SilkS) (width 0.127))
  (fp_line (start 0 -7.62) (end 12.7 -7.62) (layer F.SilkS) (width 0.127))
  (fp_line (start 12.7 -7.62) (end 12.7 -3.175) (layer F.SilkS) (width 0.127))
  (fp_line (start 0.635 1.27) (end -0.635 1.27) (layer F.SilkS) (width 0.2032))
  (fp_line (start -0.635 1.27) (end 0.635 1.27) (layer F.SilkS) (width 0.2032))
  (pad 1 thru_hole circle (at 0 -0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 2 thru_hole circle (at 2.54 0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 3 thru_hole circle (at 5.08 -0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 4 thru_hole circle (at 7.62 0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 5 thru_hole circle (at 10.16 -0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 6 thru_hole circle (at 12.7 0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
