(module MOLEX-1X2_LOCK (layer F.Cu) (tedit 5963E8A8)
  (descr "MOLEX 2-PIN PLATED THROUGH-HOLE LOCKING FOOTPRINT")
  (tags "MOLEX 2-PIN PLATED THROUGH-HOLE LOCKING FOOTPRINT")
  (attr virtual)
  (fp_text reference >NAME (at 0 -3.556) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 0 3.175) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_line (start -1.27 -3.048) (end -1.27 2.54) (layer F.SilkS) (width 0.127))
  (fp_line (start 3.81 -3.048) (end 3.81 2.54) (layer F.SilkS) (width 0.127))
  (fp_line (start 3.81 -3.048) (end -1.27 -3.048) (layer F.SilkS) (width 0.127))
  (fp_line (start 3.81 2.54) (end 2.54 2.54) (layer F.SilkS) (width 0.127))
  (fp_line (start 2.54 2.54) (end 0 2.54) (layer F.SilkS) (width 0.127))
  (fp_line (start 0 2.54) (end -1.27 2.54) (layer F.SilkS) (width 0.127))
  (fp_line (start 0 2.54) (end 0 1.27) (layer F.SilkS) (width 0.127))
  (fp_line (start 0 1.27) (end 2.54 1.27) (layer F.SilkS) (width 0.127))
  (fp_line (start 2.54 1.27) (end 2.54 2.54) (layer F.SilkS) (width 0.127))
  (pad 1 thru_hole rect (at -0.127 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 2 thru_hole circle (at 2.667 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
