(module 1X01_OFFSET (layer F.Cu) (tedit 200000)
  (descr "PLATED THROUGH HOLE - LONG PAD W/ OFFSET HOLE")
  (tags "PLATED THROUGH HOLE - LONG PAD W/ OFFSET HOLE")
  (attr virtual)
  (fp_text reference >NAME (at 0.254 -3.3528) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 0.5588 1.7272) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_line (start -0.254 0.254) (end 0.254 0.254) (layer Dwgs.User) (width 0.06604))
  (fp_line (start 0.254 0.254) (end 0.254 -0.254) (layer Dwgs.User) (width 0.06604))
  (fp_line (start -0.254 -0.254) (end 0.254 -0.254) (layer Dwgs.User) (width 0.06604))
  (fp_line (start -0.254 0.254) (end -0.254 -0.254) (layer Dwgs.User) (width 0.06604))
  (fp_line (start -1.27 -0.635) (end -1.27 0.635) (layer F.SilkS) (width 0.2032))
  (fp_line (start -1.27 0.635) (end -0.635 1.27) (layer F.SilkS) (width 0.2032))
  (fp_line (start -0.635 1.27) (end 0.635 1.27) (layer F.SilkS) (width 0.2032))
  (fp_line (start 0.635 1.27) (end 1.27 0.635) (layer F.SilkS) (width 0.2032))
  (fp_line (start 1.27 0.635) (end 1.27 -0.635) (layer F.SilkS) (width 0.2032))
  (pad 1 thru_hole rect (at 0 0) (size 1.8796 0) (drill 1.1176) (layers *.Cu *.Mask) (solder_mask_margin 0.1016))
)
