(module 1X02_BIG (layer F.Cu) (tedit 200000)
  (descr "PLATED THROUGH HOLE")
  (tags "PLATED THROUGH HOLE")
  (attr virtual)
  (fp_text reference >NAME (at 0 -1.778) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 0 1.905) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_line (start -1.27 -1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.127))
  (fp_line (start -1.27 1.27) (end 5.08 1.27) (layer F.SilkS) (width 0.127))
  (fp_line (start 5.08 1.27) (end 5.08 -1.27) (layer F.SilkS) (width 0.127))
  (fp_line (start 5.08 -1.27) (end -1.27 -1.27) (layer F.SilkS) (width 0.127))
  (pad P$1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0668) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad P$2 thru_hole circle (at 3.81 0) (size 1.6002 1.6002) (drill 1.0668) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
