(module OBDII (layer F.Cu) (tedit 5963E92B)
  (descr "OBD-II AUTOMOTIVE CONNECTOR")
  (tags "OBD-II AUTOMOTIVE CONNECTOR")
  (attr virtual)
  (fp_text reference >NAME (at 0 -7.62) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 0 6.985) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text user 1 (at 13.97 1.27) (layer F.SilkS)
    (effects (font (size 1.27 1.27) (thickness 0.2032)))
  )
  (fp_text user 16 (at -13.97 -1.905) (layer F.SilkS)
    (effects (font (size 1.27 1.27) (thickness 0.2032)))
  )
  (fp_text user 16 (at -13.97 -1.905) (layer B.SilkS)
    (effects (font (size 1.27 1.27) (thickness 0.2032)) (justify mirror))
  )
  (fp_text user 1 (at 13.97 1.27) (layer B.SilkS)
    (effects (font (size 1.27 1.27) (thickness 0.2032)) (justify mirror))
  )
  (pad 1 thru_hole circle (at 13.6779 3.81) (size 3.21564 3.21564) (drill 2.19964) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 2 thru_hole circle (at 9.7282 3.81) (size 3.21564 3.21564) (drill 2.19964) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 3 thru_hole circle (at 5.7785 3.81) (size 3.21564 3.21564) (drill 2.19964) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 4 thru_hole circle (at 1.8288 3.81) (size 3.21564 3.21564) (drill 2.19964) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 5 thru_hole circle (at -2.11836 3.81) (size 3.21564 3.21564) (drill 2.19964) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 6 thru_hole circle (at -6.06806 3.81) (size 3.21564 3.21564) (drill 2.19964) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 7 thru_hole circle (at -10.01776 3.81) (size 3.21564 3.21564) (drill 2.19964) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 8 thru_hole circle (at -13.97 3.81) (size 3.21564 3.21564) (drill 2.19964) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 9 thru_hole circle (at 13.6779 -4.58978) (size 3.21564 3.21564) (drill 2.19964) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 10 thru_hole circle (at 9.7282 -4.58978) (size 3.21564 3.21564) (drill 2.19964) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 11 thru_hole circle (at 5.7785 -4.58978) (size 3.21564 3.21564) (drill 2.19964) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 12 thru_hole circle (at 1.8288 -4.58978) (size 3.21564 3.21564) (drill 2.19964) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 13 thru_hole circle (at -2.11836 -4.58978) (size 3.21564 3.21564) (drill 2.19964) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 14 thru_hole circle (at -6.06806 -4.58978) (size 3.21564 3.21564) (drill 2.19964) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 15 thru_hole circle (at -10.01776 -4.58978) (size 3.21564 3.21564) (drill 2.19964) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 16 thru_hole circle (at -13.97 -4.58978) (size 3.21564 3.21564) (drill 2.19964) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
