(module LCD_BACKLIGHT_PADS (layer F.Cu) (tedit 200000)
  (descr "PADS FOR FLYING BACKLIGHT LEADS")
  (tags "PADS FOR FLYING BACKLIGHT LEADS")
  (attr smd)
  (fp_text reference >NAME (at -2.794 -3.175 90) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 2.794 -3.175 90) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (pad P$1 smd rect (at 0 0) (size 3.81 3.81) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad P$2 smd rect (at 0 -6.35) (size 3.81 3.81) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
)
