(module STAND-OFF-TIGHT (layer F.Cu) (tedit 200000)
  (descr "STANDOFF (#4 SCREW) - TIGHT FIT AROUND SCREW BODY")
  (tags "STANDOFF (#4 SCREW) - TIGHT FIT AROUND SCREW BODY")
  (attr virtual)
  (fp_text reference >NAME (at 0 -3.302) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 0 3.302) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_circle (center 0 0) (end 0 -2.794) (layer F.CrtYd) (width 0.127))
  (fp_arc (start 0 0) (end 0 -1.8542) (angle 180) (layer F.SilkS) (width 0.2032))
  (fp_arc (start 0 0) (end 0 1.8542) (angle 180) (layer F.SilkS) (width 0.2032))
  (fp_arc (start 0 0) (end 0 -1.8542) (angle 180) (layer F.SilkS) (width 0.2032))
  (fp_arc (start 0 0) (end 0 1.8542) (angle 180) (layer F.SilkS) (width 0.2032))
  (pad "" np_thru_hole circle (at 0 0) (size 3.048 3.048) (drill 3.048) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
