(module 1X12_HOLES_ONLY (layer F.Cu) (tedit 200000)
  (descr "HOLES -12 PIN")
  (tags "HOLES -12 PIN")
  (attr virtual)
  (fp_text reference "" (at 0 0) (layer F.SilkS)
    (effects (font (thickness 0.15)))
  )
  (fp_text value "" (at 0 0) (layer F.SilkS)
    (effects (font (thickness 0.15)))
  )
  (fp_circle (center 0 0) (end 0 -0.635) (layer Dwgs.User) (width 0.127))
  (fp_circle (center 2.54 0) (end 2.54 -0.635) (layer Dwgs.User) (width 0.127))
  (fp_circle (center 5.08 0) (end 5.08 -0.635) (layer Dwgs.User) (width 0.127))
  (fp_circle (center 7.62 0) (end 7.62 -0.635) (layer Dwgs.User) (width 0.127))
  (fp_circle (center 10.16 0) (end 10.16 -0.635) (layer Dwgs.User) (width 0.127))
  (fp_circle (center 12.7 0) (end 12.7 -0.635) (layer Dwgs.User) (width 0.127))
  (fp_circle (center 15.24 0) (end 15.24 -0.635) (layer Dwgs.User) (width 0.127))
  (fp_circle (center 17.78 0) (end 17.78 -0.635) (layer Dwgs.User) (width 0.127))
  (fp_circle (center 20.32 0) (end 20.32 -0.635) (layer Dwgs.User) (width 0.127))
  (fp_circle (center 22.86 0) (end 22.86 -0.635) (layer Dwgs.User) (width 0.127))
  (fp_circle (center 25.4 0) (end 25.4 -0.635) (layer Dwgs.User) (width 0.127))
  (fp_circle (center 27.94 0) (end 27.94 -0.635) (layer Dwgs.User) (width 0.127))
  (pad 1 thru_hole circle (at 0 0) (size 0.8128 0.8128) (drill 0.889) (layers *.Cu *.Mask) (solder_mask_margin 0.1016))
  (pad 2 thru_hole circle (at 2.54 0) (size 0.8128 0.8128) (drill 0.889) (layers *.Cu *.Mask) (solder_mask_margin 0.1016))
  (pad 3 thru_hole circle (at 5.08 0) (size 0.8128 0.8128) (drill 0.889) (layers *.Cu *.Mask) (solder_mask_margin 0.1016))
  (pad 4 thru_hole circle (at 7.62 0) (size 0.8128 0.8128) (drill 0.889) (layers *.Cu *.Mask) (solder_mask_margin 0.1016))
  (pad 5 thru_hole circle (at 10.16 0) (size 0.8128 0.8128) (drill 0.889) (layers *.Cu *.Mask) (solder_mask_margin 0.1016))
  (pad 6 thru_hole circle (at 12.7 0) (size 0.8128 0.8128) (drill 0.889) (layers *.Cu *.Mask) (solder_mask_margin 0.1016))
  (pad 7 thru_hole circle (at 15.24 0) (size 0.8128 0.8128) (drill 0.889) (layers *.Cu *.Mask) (solder_mask_margin 0.1016))
  (pad 8 thru_hole circle (at 17.78 0) (size 0.8128 0.8128) (drill 0.889) (layers *.Cu *.Mask) (solder_mask_margin 0.1016))
  (pad 9 thru_hole circle (at 20.32 0) (size 0.8128 0.8128) (drill 0.889) (layers *.Cu *.Mask) (solder_mask_margin 0.1016))
  (pad 10 thru_hole circle (at 22.86 0) (size 0.8128 0.8128) (drill 0.889) (layers *.Cu *.Mask) (solder_mask_margin 0.1016))
  (pad 11 thru_hole circle (at 25.4 0) (size 0.8128 0.8128) (drill 0.889) (layers *.Cu *.Mask) (solder_mask_margin 0.1016))
  (pad 12 thru_hole circle (at 27.94 0) (size 0.8128 0.8128) (drill 0.889) (layers *.Cu *.Mask) (solder_mask_margin 0.1016))
  (pad "" np_thru_hole circle (at 0 0) (size 1.4732 1.4732) (drill 1.4732) (layers *.Cu *.Mask) (solder_mask_margin 0.1016))
  (pad "" np_thru_hole circle (at 2.54 0) (size 1.4732 1.4732) (drill 1.4732) (layers *.Cu *.Mask) (solder_mask_margin 0.1016))
  (pad "" np_thru_hole circle (at 5.08 0) (size 1.4732 1.4732) (drill 1.4732) (layers *.Cu *.Mask) (solder_mask_margin 0.1016))
  (pad "" np_thru_hole circle (at 7.62 0) (size 1.4732 1.4732) (drill 1.4732) (layers *.Cu *.Mask) (solder_mask_margin 0.1016))
  (pad "" np_thru_hole circle (at 10.16 0) (size 1.4732 1.4732) (drill 1.4732) (layers *.Cu *.Mask) (solder_mask_margin 0.1016))
  (pad "" np_thru_hole circle (at 12.7 0) (size 1.4732 1.4732) (drill 1.4732) (layers *.Cu *.Mask) (solder_mask_margin 0.1016))
  (pad "" np_thru_hole circle (at 15.24 0) (size 1.4732 1.4732) (drill 1.4732) (layers *.Cu *.Mask) (solder_mask_margin 0.1016))
  (pad "" np_thru_hole circle (at 17.78 0) (size 1.4732 1.4732) (drill 1.4732) (layers *.Cu *.Mask) (solder_mask_margin 0.1016))
  (pad "" np_thru_hole circle (at 20.32 0) (size 1.4732 1.4732) (drill 1.4732) (layers *.Cu *.Mask) (solder_mask_margin 0.1016))
  (pad "" np_thru_hole circle (at 22.86 0) (size 1.4732 1.4732) (drill 1.4732) (layers *.Cu *.Mask) (solder_mask_margin 0.1016))
  (pad "" np_thru_hole circle (at 25.4 0) (size 1.4732 1.4732) (drill 1.4732) (layers *.Cu *.Mask) (solder_mask_margin 0.1016))
  (pad "" np_thru_hole circle (at 27.94 0) (size 1.4732 1.4732) (drill 1.4732) (layers *.Cu *.Mask) (solder_mask_margin 0.1016))
)
