(module UNO_R3_SHIELD_ICSP_NOLABELS (layer F.Cu) (tedit 200000)
  (descr "ARDUINO UNO-COMPATIBLE FOOTPRINT WITH ICSP")
  (tags "ARDUINO UNO-COMPATIBLE FOOTPRINT WITH ICSP")
  (attr virtual)
  (fp_text reference >NAME (at 0 -20.32) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 0 -19.05) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_line (start -24.13 30.48) (end -17.16786 30.48) (layer Dwgs.User) (width 0.254))
  (fp_line (start -17.16786 30.48) (end -4.96824 30.48) (layer Dwgs.User) (width 0.254))
  (fp_line (start -4.96824 30.48) (end 24.13 30.48) (layer Dwgs.User) (width 0.254))
  (fp_line (start 24.13 30.48) (end 26.67 27.94) (layer Dwgs.User) (width 0.254))
  (fp_line (start 26.67 -26.67) (end 24.13 -26.67) (layer Dwgs.User) (width 0.254))
  (fp_line (start 24.13 -26.67) (end 21.59 -29.21) (layer Dwgs.User) (width 0.254))
  (fp_line (start -26.67 -25.4) (end -26.67 27.94) (layer Dwgs.User) (width 0.254))
  (fp_line (start -26.67 27.94) (end -24.13 30.48) (layer Dwgs.User) (width 0.254))
  (fp_line (start 21.59 -29.21) (end -11.43 -29.21) (layer Dwgs.User) (width 0.254))
  (fp_line (start -11.43 -29.21) (end -13.97 -26.67) (layer Dwgs.User) (width 0.254))
  (fp_line (start -13.97 -26.67) (end -25.4 -26.67) (layer Dwgs.User) (width 0.254))
  (fp_line (start -25.4 -26.67) (end -26.67 -25.4) (layer Dwgs.User) (width 0.254))
  (fp_line (start 26.67 27.94) (end 26.67 -26.67) (layer Dwgs.User) (width 0.254))
  (fp_line (start -17.16786 45.97908) (end -4.96824 45.97908) (layer Dwgs.User) (width 0.254))
  (fp_line (start 13.52804 40.7797) (end 22.5298 40.7797) (layer Dwgs.User) (width 0.254))
  (fp_line (start -17.16786 45.97908) (end -17.16786 30.48) (layer Dwgs.User) (width 0.254))
  (fp_line (start -4.96824 45.97908) (end -4.96824 30.48) (layer Dwgs.User) (width 0.254))
  (fp_line (start 13.52804 40.7797) (end 13.52804 30.57906) (layer Dwgs.User) (width 0.254))
  (fp_line (start 22.5298 40.7797) (end 22.5298 30.57906) (layer Dwgs.User) (width 0.254))
  (fp_line (start -25.4 -25.4) (end -22.86 -25.4) (layer Dwgs.User) (width 0.127))
  (fp_line (start -22.86 -25.4) (end -22.86 -5.08) (layer Dwgs.User) (width 0.127))
  (fp_line (start -22.86 -5.08) (end -25.4 -5.08) (layer Dwgs.User) (width 0.127))
  (fp_line (start -25.4 -5.08) (end -25.4 -25.4) (layer Dwgs.User) (width 0.127))
  (fp_line (start -25.4 -3.556) (end -22.86 -3.556) (layer Dwgs.User) (width 0.127))
  (fp_line (start -22.86 -3.556) (end -22.86 21.844) (layer Dwgs.User) (width 0.127))
  (fp_line (start -22.86 21.844) (end -25.4 21.844) (layer Dwgs.User) (width 0.127))
  (fp_line (start -25.4 21.844) (end -25.4 -3.556) (layer Dwgs.User) (width 0.127))
  (fp_line (start 22.86 12.7) (end 25.4 12.7) (layer Dwgs.User) (width 0.127))
  (fp_line (start 25.4 12.7) (end 25.4 -7.62) (layer Dwgs.User) (width 0.127))
  (fp_line (start 25.4 -7.62) (end 22.86 -7.62) (layer Dwgs.User) (width 0.127))
  (fp_line (start 22.86 -7.62) (end 22.86 12.7) (layer Dwgs.User) (width 0.127))
  (fp_line (start 25.4 -10.16) (end 22.86 -10.16) (layer Dwgs.User) (width 0.127))
  (fp_line (start 22.86 -10.16) (end 22.86 -25.4) (layer Dwgs.User) (width 0.127))
  (fp_line (start 22.86 -25.4) (end 25.4 -25.4) (layer Dwgs.User) (width 0.127))
  (fp_line (start 25.4 -25.4) (end 25.4 -10.16) (layer Dwgs.User) (width 0.127))
  (fp_line (start -4.445 -22.987) (end -5.08 -23.622) (layer Dwgs.User) (width 0.254))
  (fp_line (start -5.08 -23.622) (end -5.08 -27.432) (layer Dwgs.User) (width 0.254))
  (fp_line (start -5.08 -27.432) (end -4.445 -28.067) (layer Dwgs.User) (width 0.254))
  (fp_line (start -4.445 -28.067) (end 2.032 -28.067) (layer Dwgs.User) (width 0.254))
  (fp_line (start 2.032 -28.067) (end 2.667 -27.432) (layer Dwgs.User) (width 0.254))
  (fp_line (start 2.667 -27.432) (end 2.667 -23.622) (layer Dwgs.User) (width 0.254))
  (fp_line (start 2.667 -23.622) (end 2.032 -22.987) (layer Dwgs.User) (width 0.254))
  (fp_line (start 2.032 -22.987) (end -4.445 -22.987) (layer Dwgs.User) (width 0.254))
  (fp_line (start -3.175 -22.479) (end -4.445 -22.479) (layer Dwgs.User) (width 0.2032))
  (fp_text user GND (at 21.2217 -1.27 180) (layer Dwgs.User)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user GND (at 21.2217 -3.81 180) (layer Dwgs.User)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user +5V (at 21.2217 1.27 180) (layer Dwgs.User)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user RST (at 21.2217 6.35 180) (layer Dwgs.User)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user VIN (at 21.2217 -6.35 180) (layer Dwgs.User)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user +3.3V (at 20.2057 3.81 180) (layer Dwgs.User)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user 0 (at 22.2377 -11.43 180) (layer Dwgs.User)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user 1 (at 22.2377 -13.97 180) (layer Dwgs.User)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user 2 (at 22.2377 -16.51 180) (layer Dwgs.User)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user 3 (at 22.2377 -19.05 180) (layer Dwgs.User)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user 4 (at 22.2377 -21.59 180) (layer Dwgs.User)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user 5 (at 22.2377 -24.13 180) (layer Dwgs.User)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user "Analog In" (at 20.7137 -17.145 270) (layer Dwgs.User)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user GND (at -21.336 12.954) (layer Dwgs.User)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user 13 (at -21.844 10.414) (layer Dwgs.User)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user 12 (at -21.844 7.874) (layer Dwgs.User)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user 11 (at -21.844 5.334) (layer Dwgs.User)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user AREF (at -20.828 15.494) (layer Dwgs.User)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user 10 (at -21.844 2.794) (layer Dwgs.User)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user 9 (at -22.352 0.254) (layer Dwgs.User)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user 8 (at -22.352 -2.286) (layer Dwgs.User)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user 7 (at -22.352 -6.35) (layer Dwgs.User)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user 6 (at -22.352 -8.89) (layer Dwgs.User)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user 5 (at -22.352 -11.43) (layer Dwgs.User)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user 4 (at -22.352 -13.97) (layer Dwgs.User)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user 3 (at -22.352 -16.51) (layer Dwgs.User)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user 2 (at -22.352 -19.05) (layer Dwgs.User)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user TX (at -21.844 -21.59) (layer Dwgs.User)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user RX (at -21.844 -24.13) (layer Dwgs.User)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user SDA (at -21.336 18.034) (layer Dwgs.User)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user SCL (at -21.336 20.574) (layer Dwgs.User)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user IOREF (at 20.2057 8.89 180) (layer Dwgs.User)
    (effects (font (size 1.016 1.016) (thickness 0.1524)))
  )
  (fp_text user USB (at -10.2108 44.0436) (layer Dwgs.User)
    (effects (font (size 0.8128 0.8128) (thickness 0.1524)))
  )
  (fp_text user "PWR JACK" (at 21.0312 38.9636) (layer Dwgs.User)
    (effects (font (size 0.8128 0.8128) (thickness 0.1524)))
  )
  (pad 3.3V thru_hole circle (at 24.13 3.81) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 5V thru_hole circle (at 24.13 1.27) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 5V_I thru_hole circle (at -3.7592 -26.8097) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad A0 thru_hole circle (at 24.13 -11.43) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad A1 thru_hole circle (at 24.13 -13.97) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad A2 thru_hole circle (at 24.13 -16.51) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad A3 thru_hole circle (at 24.13 -19.05) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad A4 thru_hole circle (at 24.13 -21.59) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad A5 thru_hole circle (at 24.13 -24.13) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad AREF thru_hole circle (at -24.13 15.494) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad D2 thru_hole circle (at -24.13 -19.05) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad D3 thru_hole circle (at -24.13 -16.51) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad D4 thru_hole circle (at -24.13 -13.97) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad D5 thru_hole circle (at -24.13 -11.43) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad D6 thru_hole circle (at -24.13 -8.89) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad D7 thru_hole circle (at -24.13 -6.35) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad D8 thru_hole circle (at -24.13 -2.286) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad D9 thru_hole circle (at -24.13 0.254) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad D10 thru_hole circle (at -24.13 2.794) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad D11 thru_hole circle (at -24.13 5.334) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad D12 thru_hole circle (at -24.13 7.874) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad D13 thru_hole circle (at -24.13 10.414) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad GND@ thru_hole circle (at 24.13 -1.27) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad GND@ thru_hole circle (at 24.13 -3.81) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad GND@ thru_hole circle (at -24.13 12.954) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad GND_ thru_hole circle (at 1.31826 -26.8097) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad IORE thru_hole circle (at 24.13 8.89) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad MISO thru_hole circle (at -3.7592 -24.2697) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad MOSI thru_hole circle (at -1.2192 -26.8097) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad NC thru_hole circle (at 24.13 11.43) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad RES thru_hole circle (at 24.13 6.35) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad RST_ thru_hole circle (at 1.31826 -24.2697) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad RX thru_hole circle (at -24.13 -24.13) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad SCK thru_hole circle (at -1.2192 -24.2697) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad SCL thru_hole circle (at -24.13 20.574) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad SDA thru_hole circle (at -24.13 18.034) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad TX thru_hole circle (at -24.13 -21.59) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad VIN thru_hole circle (at 24.13 -6.35) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
