(module 1X24_LONGPADS (layer F.Cu) (tedit 5963DCAA)
  (descr "PLATED THROUGH HOLE -24 PIN LONG PADS")
  (tags "PLATED THROUGH HOLE -24 PIN LONG PADS")
  (attr virtual)
  (fp_text reference >NAME (at -26.67 -2.54) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at -26.67 2.54) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_line (start 33.02 -0.635) (end 33.02 0.635) (layer F.SilkS) (width 0.2032))
  (fp_line (start -27.94 -0.635) (end -27.94 0.635) (layer F.SilkS) (width 0.2032))
  (pad 2 thru_hole oval (at -26.67 0 180) (size 1.8796 3.7592) (drill 1.1176) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 3 thru_hole oval (at -24.13 0 180) (size 1.8796 3.7592) (drill 1.1176) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 4 thru_hole oval (at -21.59 0 180) (size 1.8796 3.7592) (drill 1.1176) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 5 thru_hole oval (at -19.05 0 180) (size 1.8796 3.7592) (drill 1.1176) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 6 thru_hole oval (at -16.51 0 180) (size 1.8796 3.7592) (drill 1.1176) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 7 thru_hole oval (at -13.97 0 180) (size 1.8796 3.7592) (drill 1.1176) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 8 thru_hole oval (at -11.43 0 180) (size 1.8796 3.7592) (drill 1.1176) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 9 thru_hole oval (at -8.89 0 180) (size 1.8796 3.7592) (drill 1.1176) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 10 thru_hole oval (at -6.35 0 180) (size 1.8796 3.7592) (drill 1.1176) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 11 thru_hole oval (at -3.81 0 180) (size 1.8796 3.7592) (drill 1.1176) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 12 thru_hole oval (at -1.27 0 180) (size 1.8796 3.7592) (drill 1.1176) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 13 thru_hole oval (at 1.27 0 180) (size 1.8796 3.7592) (drill 1.1176) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 14 thru_hole oval (at 3.81 0 180) (size 1.8796 3.7592) (drill 1.1176) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 15 thru_hole oval (at 6.35 0 180) (size 1.8796 3.7592) (drill 1.1176) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 16 thru_hole oval (at 8.89 0 180) (size 1.8796 3.7592) (drill 1.1176) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 17 thru_hole oval (at 11.43 0 180) (size 1.8796 3.7592) (drill 1.1176) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 18 thru_hole oval (at 13.97 0 180) (size 1.8796 3.7592) (drill 1.1176) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 19 thru_hole oval (at 16.51 0 180) (size 1.8796 3.7592) (drill 1.1176) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 20 thru_hole oval (at 19.05 0 180) (size 1.8796 3.7592) (drill 1.1176) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 21 thru_hole oval (at 21.59 0 180) (size 1.8796 3.7592) (drill 1.1176) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 22 thru_hole oval (at 24.13 0 180) (size 1.8796 3.7592) (drill 1.1176) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 23 thru_hole oval (at 26.67 0 180) (size 1.8796 3.7592) (drill 1.1176) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 24 thru_hole oval (at 29.21 0 180) (size 1.8796 3.7592) (drill 1.1176) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 25 thru_hole oval (at 31.75 0 180) (size 1.8796 3.7592) (drill 1.1176) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
