(module PCB_MOUNT_SPEAKER (layer F.Cu) (tedit 200000)
  (descr "SPEAKER - PCB MOUNT")
  (tags "SPEAKER - PCB MOUNT")
  (attr virtual)
  (fp_text reference >NAME (at 0 -15.24) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 0 15.367) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_circle (center 0 0) (end 0 -14.605) (layer F.SilkS) (width 0.2032))
  (pad + thru_hole rect (at -7.62 0) (size 1.7145 1.7145) (drill 1.143) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad - thru_hole rect (at 7.62 0) (size 1.7145 1.7145) (drill 1.143) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
