(module TQFP64_14X14MM (layer F.Cu) (tedit 200000)
  (descr "64-LEAD TQFP PLASTIC THIN QUAD FLATPACK - 14X14X1MM BODY")
  (tags "64-LEAD TQFP PLASTIC THIN QUAD FLATPACK - 14X14X1MM BODY")
  (attr smd)
  (fp_text reference >NAME (at -9.017 0 90) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 9.144 0 90) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_circle (center -7.239 7.239) (end -6.985 7.239) (layer F.SilkS) (width 0.254))
  (fp_circle (center -7.239 7.239) (end -7.112 7.239) (layer F.SilkS) (width 0.254))
  (fp_line (start 6.9977 -6.9977) (end -6.9977 -6.9977) (layer Dwgs.User) (width 0.127))
  (fp_line (start -6.9977 -6.9977) (end -6.9977 6.9977) (layer Dwgs.User) (width 0.127))
  (fp_line (start -6.9977 6.9977) (end 6.9977 6.9977) (layer Dwgs.User) (width 0.127))
  (fp_line (start 6.9977 6.9977) (end 6.9977 -6.9977) (layer Dwgs.User) (width 0.127))
  (fp_line (start -7.0993 -6.39826) (end -7.0993 -7.0993) (layer F.SilkS) (width 0.127))
  (fp_line (start -7.0993 -7.0993) (end -6.39826 -7.0993) (layer F.SilkS) (width 0.127))
  (fp_line (start 6.39826 -7.0993) (end 7.0993 -7.0993) (layer F.SilkS) (width 0.127))
  (fp_line (start 7.0993 -7.0993) (end 7.0993 -6.39826) (layer F.SilkS) (width 0.127))
  (fp_line (start 7.0993 6.39826) (end 7.0993 7.0993) (layer F.SilkS) (width 0.127))
  (fp_line (start 7.0993 7.0993) (end 6.39826 7.0993) (layer F.SilkS) (width 0.127))
  (fp_line (start -6.9977 6.39826) (end -6.39826 6.9977) (layer F.SilkS) (width 0.127))
  (pad 1 smd rect (at -5.99948 7.59968 90) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 2 smd rect (at -5.19938 7.59968 90) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 3 smd rect (at -4.39928 7.59968 90) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 4 smd rect (at -3.59918 7.59968 90) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 5 smd rect (at -2.79908 7.59968 90) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 6 smd rect (at -1.99898 7.59968 90) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 7 smd rect (at -1.19888 7.59968 90) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 8 smd rect (at -0.39878 7.59968 90) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 9 smd rect (at 0.39878 7.59968 90) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 10 smd rect (at 1.19888 7.59968 90) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 11 smd rect (at 1.99898 7.59968 90) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 12 smd rect (at 2.79908 7.59968 90) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 13 smd rect (at 3.59918 7.59968 90) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 14 smd rect (at 4.39928 7.59968 90) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 15 smd rect (at 5.19938 7.59968 90) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 16 smd rect (at 5.99948 7.59968 90) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 17 smd rect (at 7.59968 5.99948 180) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 18 smd rect (at 7.59968 5.19938 180) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 19 smd rect (at 7.59968 4.39928 180) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 20 smd rect (at 7.59968 3.59918 180) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 21 smd rect (at 7.59968 2.79908 180) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 22 smd rect (at 7.59968 1.99898 180) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 23 smd rect (at 7.59968 1.19888 180) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 24 smd rect (at 7.59968 0.39878 180) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 25 smd rect (at 7.59968 -0.39878 180) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 26 smd rect (at 7.59968 -1.19888 180) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 27 smd rect (at 7.59968 -1.99898 180) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 28 smd rect (at 7.59968 -2.79908 180) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 29 smd rect (at 7.59968 -3.59918 180) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 30 smd rect (at 7.59968 -4.39928 180) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 31 smd rect (at 7.59968 -5.19938 180) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 32 smd rect (at 7.59968 -5.99948 180) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 33 smd rect (at 5.99948 -7.59968 270) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 34 smd rect (at 5.19938 -7.59968 270) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 35 smd rect (at 4.39928 -7.59968 270) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 36 smd rect (at 3.59918 -7.59968 270) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 37 smd rect (at 2.79908 -7.59968 270) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 38 smd rect (at 1.99898 -7.59968 270) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 39 smd rect (at 1.19888 -7.59968 270) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 40 smd rect (at 0.39878 -7.59968 270) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 41 smd rect (at -0.39878 -7.59968 270) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 42 smd rect (at -1.19888 -7.59968 270) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 43 smd rect (at -1.99898 -7.59968 270) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 44 smd rect (at -2.79908 -7.59968 270) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 45 smd rect (at -3.59918 -7.59968 270) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 46 smd rect (at -4.39928 -7.59968 270) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 47 smd rect (at -5.19938 -7.59968 270) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 48 smd rect (at -5.99948 -7.59968 270) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 49 smd rect (at -7.59968 -5.99948) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 50 smd rect (at -7.59968 -5.19938) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 51 smd rect (at -7.59968 -4.39928) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 52 smd rect (at -7.59968 -3.59918) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 53 smd rect (at -7.59968 -2.79908) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 54 smd rect (at -7.59968 -1.99898) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 55 smd rect (at -7.59968 -1.19888) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 56 smd rect (at -7.59968 -0.39878) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 57 smd rect (at -7.59968 0.39878) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 58 smd rect (at -7.59968 1.19888) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 59 smd rect (at -7.59968 1.99898) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 60 smd rect (at -7.59968 2.79908) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 61 smd rect (at -7.59968 3.59918) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 62 smd rect (at -7.59968 4.39928) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 63 smd rect (at -7.59968 5.19938) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 64 smd rect (at -7.59968 5.99948) (size 1.27 0.39878) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
)
