(module SCREENKEY_MATING_CONNECTOR (layer F.Cu) (tedit 200000)
  (descr "FPC/FFC LOCKING CONNECTOR - SMD")
  (tags "FPC/FFC LOCKING CONNECTOR - SMD")
  (attr smd)
  (fp_text reference >NAME (at -0.635 -0.381 90) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 10.795 -0.254 90) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_line (start 0 -0.127) (end 9.99998 -0.127) (layer F.SilkS) (width 0.2032))
  (fp_line (start 9.99998 -0.127) (end 9.99998 -2.032) (layer F.SilkS) (width 0.2032))
  (fp_line (start 9.99998 -3.7846) (end 9.99998 -5.4991) (layer F.SilkS) (width 0.2032))
  (fp_line (start 9.99998 -5.4991) (end 0 -5.4991) (layer F.SilkS) (width 0.2032))
  (fp_line (start 0 -2.1082) (end 0 -0.127) (layer F.SilkS) (width 0.2032))
  (fp_line (start 0 -5.4864) (end 0 -3.937) (layer F.SilkS) (width 0.2032))
  (pad 1 smd rect (at 1.75768 0.35814 180) (size 0.19812 0.49784) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 2 smd rect (at 2.25806 0.35814 180) (size 0.19812 0.49784) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 3 smd rect (at 2.75844 0.35814 180) (size 0.19812 0.49784) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 4 smd rect (at 3.25882 0.35814 180) (size 0.19812 0.49784) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 5 smd rect (at 3.7592 0.35814 180) (size 0.19812 0.49784) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 6 smd rect (at 4.25958 0.35814 180) (size 0.19812 0.49784) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 7 smd rect (at 4.75996 0.35814 180) (size 0.19812 0.49784) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 8 smd rect (at 5.2578 0.35814 180) (size 0.19812 0.49784) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 9 smd rect (at 5.75818 0.35814 180) (size 0.19812 0.49784) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 10 smd rect (at 6.25856 0.35814 180) (size 0.19812 0.49784) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 11 smd rect (at 6.75894 0.35814 180) (size 0.19812 0.49784) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 12 smd rect (at 7.25932 0.35814 180) (size 0.19812 0.49784) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 13 smd rect (at 7.7597 0.35814 180) (size 0.19812 0.49784) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 14 smd rect (at 8.25754 0.35814 180) (size 0.19812 0.49784) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad P$15 smd rect (at 0 -2.99974) (size 1.27762 1.27762) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad P$16 smd rect (at 10.09904 -2.89814) (size 1.27762 1.27762) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
)
