(module 2X3_SMT_POSTS (layer F.Cu) (tedit 200000)
  (descr "SURFACE MOUNT - 2X3 MALE HEADER WITH KEYING POSTS")
  (tags "SURFACE MOUNT - 2X3 MALE HEADER WITH KEYING POSTS")
  (attr smd)
  (fp_text reference >NAME (at -2.54 -4.7498) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at -2.54 4.7752) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_line (start -1.778 -2.54) (end -0.762 -2.54) (layer F.SilkS) (width 0.2032))
  (fp_line (start 0.762 -2.54) (end 1.778 -2.54) (layer F.SilkS) (width 0.2032))
  (fp_line (start -1.778 2.54) (end -0.889 2.54) (layer F.SilkS) (width 0.2032))
  (fp_line (start 0.762 2.54) (end 1.778 2.54) (layer F.SilkS) (width 0.2032))
  (fp_line (start -3.175 -2.54) (end -3.81 -2.54) (layer F.SilkS) (width 0.2032))
  (fp_line (start -3.81 -2.54) (end -3.81 2.54) (layer F.SilkS) (width 0.2032))
  (fp_line (start -3.81 2.54) (end -3.175 2.54) (layer F.SilkS) (width 0.2032))
  (fp_line (start 3.175 -2.54) (end 3.81 -2.54) (layer F.SilkS) (width 0.2032))
  (fp_line (start 3.81 -2.54) (end 3.81 2.54) (layer F.SilkS) (width 0.2032))
  (fp_line (start 3.81 2.54) (end 3.175 2.54) (layer F.SilkS) (width 0.2032))
  (fp_line (start -3.429 4.064) (end -3.429 2.794) (layer F.SilkS) (width 0.2032))
  (pad 1 smd rect (at -2.54 2.54 90) (size 3.16992 0.99822) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 2 smd rect (at -2.54 -2.54 90) (size 3.16992 0.99822) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 3 smd rect (at 0 2.54 90) (size 3.16992 0.99822) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 4 smd rect (at 0 -2.54 90) (size 3.16992 0.99822) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 5 smd rect (at 2.54 2.54 90) (size 3.16992 0.99822) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 6 smd rect (at 2.54 -2.54 90) (size 3.16992 0.99822) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad "" np_thru_hole circle (at -1.27 0) (size 1.79832 1.79832) (drill 1.79832) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad "" np_thru_hole circle (at 1.27 0) (size 1.79832 1.79832) (drill 1.79832) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
