(module T5403 (layer F.Cu) (tedit 200000)
  (descr "T5400, T54003 DIGITAL BAROMETRIC PRESSURE SENSOR")
  (tags "T5400, T54003 DIGITAL BAROMETRIC PRESSURE SENSOR")
  (attr smd)
  (fp_text reference >NAME (at 0 -1.778) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 0 1.778) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_circle (center -1.905 1.27) (end -1.778 1.27) (layer F.SilkS) (width 0.254))
  (fp_line (start -1.4732 -1.2192) (end -1.4732 1.2192) (layer F.SilkS) (width 0.2032))
  (fp_line (start -1.4732 -1.2192) (end 1.49098 -1.2192) (layer F.SilkS) (width 0.2032))
  (fp_line (start -1.4732 1.2192) (end 1.49098 1.2192) (layer F.SilkS) (width 0.2032))
  (fp_line (start 1.49098 1.2192) (end 1.49098 -1.2192) (layer F.SilkS) (width 0.2032))
  (fp_circle (center -1.8542 0.889) (end -1.8542 0.635) (layer F.SilkS) (width 0))
  (pad 1 smd rect (at -1.06426 0.62484) (size 0.4191 0.79756) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 2 smd rect (at -0.35306 0.7493) (size 0.4191 0.54864) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 3 smd rect (at 0.35306 0.7493) (size 0.4191 0.54864) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 4 smd rect (at 1.06426 0.7493) (size 0.4191 0.54864) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 5 smd rect (at 1.06426 -0.7493) (size 0.4191 0.54864) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 6 smd rect (at 0.35306 -0.7493) (size 0.4191 0.54864) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 7 smd rect (at -0.35306 -0.7493) (size 0.4191 0.54864) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 8 smd rect (at -1.06426 -0.7493) (size 0.4191 0.54864) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
)
