(module TACTILE_SWITCH_SMD_5.2MM (layer F.Cu) (tedit 200000)
  (descr "MOMENTARY SWITCH (PUSHBUTTON) - SPST - SMD, 5.2MM SQUARE")
  (tags "MOMENTARY SWITCH (PUSHBUTTON) - SPST - SMD, 5.2MM SQUARE")
  (attr smd)
  (fp_text reference >NAME (at 0 -3.175) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 0 3.175) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_line (start -1.53924 2.54) (end -2.54 1.53924) (layer Dwgs.User) (width 0.2032))
  (fp_line (start -2.54 1.23952) (end -2.54 -1.27) (layer F.SilkS) (width 0.2032))
  (fp_line (start -2.54 -1.53924) (end -1.53924 -2.54) (layer Dwgs.User) (width 0.2032))
  (fp_line (start -1.53924 -2.54) (end 1.53924 -2.54) (layer F.SilkS) (width 0.2032))
  (fp_line (start 1.53924 -2.54) (end 2.54 -1.53924) (layer Dwgs.User) (width 0.2032))
  (fp_line (start 2.54 -1.23952) (end 2.54 1.23952) (layer F.SilkS) (width 0.2032))
  (fp_line (start 2.54 1.53924) (end 1.53924 2.54) (layer Dwgs.User) (width 0.2032))
  (fp_line (start 1.53924 2.54) (end -1.53924 2.54) (layer F.SilkS) (width 0.2032))
  (fp_line (start 1.905 -1.27) (end 1.905 -0.4445) (layer Dwgs.User) (width 0.127))
  (fp_line (start 1.905 -0.4445) (end 2.159 0.00762) (layer Dwgs.User) (width 0.127))
  (fp_line (start 1.905 0.2286) (end 1.905 1.11252) (layer Dwgs.User) (width 0.127))
  (fp_circle (center 0 0) (end 0 -1.27) (layer F.SilkS) (width 0.2032))
  (pad 1 smd rect (at -2.794 -1.905 90) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 2 smd rect (at 2.794 -1.905 90) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 3 smd rect (at -2.794 1.905 90) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad 4 smd rect (at 2.794 1.905 90) (size 0.762 1.524) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
)
