EESchema-DOCLIB  Version 2.0
#
$CMP AD8045-PAD
D Unity-gain stable feedback amplifier Low noise, low distortion, 1GHz BW.  <a href="https://cdn.sparkfun.com/datasheets/BreakoutBoards/AD8045.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/11420">SparkFun MiniGen - Pro Mini Signal Generator Shield</a> (BOB-11420)</li></ul><br>
K PROD_ID:IC-11224
$ENDCMP
#
$CMP AD8607
D Micropower Low-noise Rail to Rail OP-AMP  <a href="">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href=""></a> ()</li></ul><br>Currently in prototype (unknown project) 
K PROD_ID:IC-13133
$ENDCMP
#
$CMP LM339
D Quad Comparator - LM339PWR Based on information from the SLCS006N datasheet from TI (www.ti.com). Created by nick@scantool.net, 2008.  Updated 2016. <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/9555">SparkFun OBD-II UART</a> (WIG-09555)</li><li><a href="https://www.sparkfun.com/products/10769">SparkFun Car Diagnostics Kit</a> (RTL-10769)</li></ul>
K PROD_ID:IC-09990
$ENDCMP
#
$CMP LM358
D LM358 Jellybean op-amp<a href="http://www.sparkfun.com/datasheets/Components/General/LM358.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/9456">Op-Amp (Thru-Hole) - LM358</a> (COM-09456)</li></ul>
K PROD_ID:IC-09172
$ENDCMP
#
$CMP LM358KIT
D LM358 Jellybean op-amp<a href="http://www.sparkfun.com/datasheets/Components/General/LM358.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/9456">Op-Amp (Thru-Hole) - LM358</a> (COM-09456)</li></ul>
K PROD_ID:IC-09172
$ENDCMP
#
$CMP LM386
D low voltage audio power amplifier  <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/11043">FabFM Radio Kit</a> (KIT-11043)</li></ul>
K PROD_ID:IC-10899
$ENDCMP
#
$CMP LMV324
D IC LMV324 Quad Op Amp  Jellybean quad op-amp <a href="http://cdn.sparkfun.com/datasheets/Sensors/Sound/LMV324.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/13754">SparkFun Sensor Kit</a> (DEV-13754)</li><li><a href="https://www.sparkfun.com/products/13844">SparkFun Inventor's Kit for Arduino 101</a> (KIT-13844)</li><li><a href="https://www.sparkfun.com/products/12642">SparkFun Sound Detector</a> (SEN-12642)</li></ul>
K PROD_ID:IC-08227
$ENDCMP
#
$CMP LMV358SOIC
D IC LMV358 DUAL OP AMP Jellybean rail-to-rail output op-amp <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/11888">SparkFun PicoBoard</a> (WIG-11888)</li><li><a href="https://www.sparkfun.com/products/12858">SparkFun Vernier Interface Shield</a> (DEV-12858)</li><li><a href="https://www.sparkfun.com/products/13794">SparkFun Blynk Board - ESP8266</a> (WRL-13794)</li><li><a href="https://www.sparkfun.com/products/12651">SparkFun Digital Sandbox</a> (DEV-12651 RoHS)</li></ul>
K PROD_ID:IC-09657
$ENDCMP
#
$CMP MCP6021T-E_OT
D MCP6021T-E/OT OP AMP Rail-to-rail input/output op-amp with 10 MHz bandwidth. <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/12780">ZX Distance and Gesture Sensor</a> (SEN-12780)</li></ul>
K PROD_ID:IC-12504
$ENDCMP
#
$CMP OPA344
D  Single gate rail-to-rail output op-amp. Inputs extend 300mV past rails. <a href="http://www.ti.com/product/OPA344">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/8883">SparkFun Low Current Sensor</a> (SEN-08883)</li><li><a href="https://www.sparkfun.com/products/12758">SparkFun Electret Microphone Breakout</a> (BOB-12758)</li></ul>
K PROD_ID:IC-08251
$ENDCMP
#
$CMP OPAMP-DUAL
D Generic op-amp footprint This component is for the standard 358 pinning of a dual op-amp From the LM358 datasheet:<ul><li>Pin 1: Output A</li><li>Pin 2: Inverting Input A</li><li>Pin 3: Non-Inverting Input A</li><li>Pin 4: Gnd</li><li>Pin 5: Non-Inverting Input B</li><li>Pin 6: Inverting Input B</li><li>Pin 7: Output B</li><li>Pin 8: V+</li></ul>
K PROD_ID:NA-XXXXX
$ENDCMP
#
$CMP OPAMP-DUALU
D Generic op-amp footprint This component is for the standard 358 pinning of a dual op-amp From the LM358 datasheet:<ul><li>Pin 1: Output A</li><li>Pin 2: Inverting Input A</li><li>Pin 3: Non-Inverting Input A</li><li>Pin 4: Gnd</li><li>Pin 5: Non-Inverting Input B</li><li>Pin 6: Inverting Input B</li><li>Pin 7: Output B</li><li>Pin 8: V+</li></ul>
K PROD_ID:NA-XXXXX
$ENDCMP
#
$CMP TPA2005D1DGN
D 1.4W MONO CLASS-D AUDIO POWER AMPLIFIER The TPA2005D1 is a 1.4-W high efficiency filter-free class-D audio power amplifier in a BGA, QFN, or MSOP package that requires only three external components. Datasheet: <a href="http://focus.ti.com/lit/ds/symlink/tpa2005d1.pdf">http://focus.ti.com/lit/ds/symlink/tpa2005d1.pdf</a> <ul><li>1.4 W Into 8 ? From a 5V Supply at THD = 10% (Typ)</li><li>Maximum Battery Life and Minimum Heat</li><li>Efficiency With an 8-? Speaker: 84% at 400 mW, 79% at 100 mW</li><li>2.8-mA Quiescent Current</li><li>0.5-mA Shutdown Current</li><li>Ideal for Wireless or Cellular Handsets and PDAs</li><li>Capable of Driving an 8-? Speaker (2.5 V ? VDD ? 5.5 V) and a 4-? Speaker (2.5 V ? VDD ? 4.2 V)</li><li>Only Three External Components</li><li>Optimized PWM Output Stage Eliminates LC Output Filter</li><li>Internally Generated 250-kHz Switching Frequency Eliminates Capacitor and Resistor</li><li>Improved PSRR (-71 dB at 217 Hz) and Wide Supply Voltage (2.5 V to 5.5 V) Eliminates Need for a Voltage Regulator</li><li>Fully Differential Design Reduces RF Rectification and Eliminates Bypass Capacitor</li><li>Improved CMRR Eliminates Two Input Coupling Capacitors</li></ul><h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/11044">SparkFun Mono Audio Amp Breakout - TPA2005D1</a> (BOB-11044)</li></ul>Note:  SparkFun currenly only uses the QFN style part
K PROD_ID:NA-XXXXX
$ENDCMP
#
$CMP TPA2005D1DRB
D 1.4W MONO CLASS-D AUDIO POWER AMPLIFIER The TPA2005D1 is a 1.4-W high efficiency filter-free class-D audio power amplifier in a BGA, QFN, or MSOP package that requires only three external components. Datasheet: <a href="http://focus.ti.com/lit/ds/symlink/tpa2005d1.pdf">http://focus.ti.com/lit/ds/symlink/tpa2005d1.pdf</a> <ul><li>1.4 W Into 8 ? From a 5V Supply at THD = 10% (Typ)</li><li>Maximum Battery Life and Minimum Heat</li><li>Efficiency With an 8-? Speaker: 84% at 400 mW, 79% at 100 mW</li><li>2.8-mA Quiescent Current</li><li>0.5-mA Shutdown Current</li><li>Ideal for Wireless or Cellular Handsets and PDAs</li><li>Capable of Driving an 8-? Speaker (2.5 V ? VDD ? 5.5 V) and a 4-? Speaker (2.5 V ? VDD ? 4.2 V)</li><li>Only Three External Components</li><li>Optimized PWM Output Stage Eliminates LC Output Filter</li><li>Internally Generated 250-kHz Switching Frequency Eliminates Capacitor and Resistor</li><li>Improved PSRR (-71 dB at 217 Hz) and Wide Supply Voltage (2.5 V to 5.5 V) Eliminates Need for a Voltage Regulator</li><li>Fully Differential Design Reduces RF Rectification and Eliminates Bypass Capacitor</li><li>Improved CMRR Eliminates Two Input Coupling Capacitors</li></ul><h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/11044">SparkFun Mono Audio Amp Breakout - TPA2005D1</a> (BOB-11044)</li></ul>Note:  SparkFun currenly only uses the QFN style part
K PROD_ID:IC-10975
$ENDCMP
#
$CMP TPA6111SMD-T
D TPA6111A2 Basic 150mW stereo headphone amplifier. <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/12938">SparkFun FM Tuner Evaluation Board - Si4703</a> (WRL-12938)</li></ul>
K PROD_ID:IC-10149
$ENDCMP
#
$CMP TPA6138A2
D Headphone driver amp Differential to single-ended audio amplifier. <a href="">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/11924">SparkFun Purpletooth Jamboree - BC127 Development Board</a> (WRL-11924)</li></ul>
K PROD_ID:IC-11779
$ENDCMP
#
#End Doc Library
