(module JST-2-PTH (layer F.Cu) (tedit 200000)
  (descr "JST 2 PIN RIGHT ANGLE PLATED THROUGH  HOLE")
  (tags "JST 2 PIN RIGHT ANGLE PLATED THROUGH  HOLE")
  (attr virtual)
  (fp_text reference >NAME (at -3.556 0 90) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 3.556 0 90) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_line (start -2.94894 1.59766) (end -2.94894 -5.99948) (layer F.SilkS) (width 0.2032))
  (fp_line (start -2.94894 -5.99948) (end 2.94894 -5.99948) (layer F.SilkS) (width 0.2032))
  (fp_line (start 2.94894 -5.99948) (end 2.94894 1.59766) (layer F.SilkS) (width 0.2032))
  (fp_line (start -2.94894 1.59766) (end -2.2987 1.59766) (layer F.SilkS) (width 0.2032))
  (fp_line (start 2.94894 1.59766) (end 2.2987 1.59766) (layer F.SilkS) (width 0.2032))
  (fp_line (start -2.2987 1.59766) (end -2.2987 0) (layer F.SilkS) (width 0.2032))
  (fp_line (start 2.2987 1.59766) (end 2.2987 0) (layer F.SilkS) (width 0.2032))
  (fp_text user + (at 1.23444 -1.3335) (layer Dwgs.User)
    (effects (font (size 1.27 1.27) (thickness 0.1016)))
  )
  (fp_text user - (at -0.76454 -1.3335) (layer Dwgs.User)
    (effects (font (size 1.27 1.27) (thickness 0.1016)))
  )
  (pad 1 thru_hole circle (at -0.99822 0) (size 1.59766 1.59766) (drill 0.6985) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 2 thru_hole circle (at 0.99822 0) (size 1.59766 1.59766) (drill 0.6985) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
