(module PHOTOCELL-KIT (layer F.Cu) (tedit 5963C708)
  (descr "CDS PHOTOCOUNDUCTIVE PHOTOCELL (PTH) - KIT")
  (tags "CDS PHOTOCOUNDUCTIVE PHOTOCELL (PTH) - KIT")
  (attr virtual)
  (fp_text reference >NAME (at 0 -2.54) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 0 2.667) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_line (start -0.99822 -1.99898) (end 0.99822 -1.99898) (layer F.SilkS) (width 0.2032))
  (fp_line (start 0.99822 1.99898) (end -0.99822 1.99898) (layer F.SilkS) (width 0.2032))
  (fp_arc (start -1.00584 0.74676) (end -0.99822 1.99898) (angle 72.6) (layer F.SilkS) (width 0.2032))
  (fp_arc (start 1.00584 0.74676) (end 2.1971 1.12776) (angle 72.6) (layer F.SilkS) (width 0.2032))
  (fp_arc (start -1.00584 -0.74676) (end -2.1971 -1.12776) (angle 72.6) (layer F.SilkS) (width 0.2032))
  (fp_arc (start 1.00584 -0.74676) (end 0.99822 -1.99898) (angle 72.6) (layer F.SilkS) (width 0.2032))
  (pad 1 thru_hole circle (at -1.99898 0) (size 1.8796 1.8796) (drill 0.89916) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 2 thru_hole circle (at 1.99898 0) (size 1.8796 1.8796) (drill 0.89916) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
