(module 1X04_LOCK_LONGPADS (layer F.Cu) (tedit 5963D329)
  (descr "PLATED THROUGH HOLE - 4 PIN LONG PADS W/ LOCKING FOOTPRINT")
  (tags "PLATED THROUGH HOLE - 4 PIN LONG PADS W/ LOCKING FOOTPRINT")
  (attr virtual)
  (fp_text reference >NAME (at 0 -2.159) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at -0.127 2.286) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_line (start 1.524 0.127) (end 1.016 0.127) (layer F.SilkS) (width 0.2032))
  (fp_line (start 4.064 0.127) (end 3.556 0.127) (layer F.SilkS) (width 0.2032))
  (fp_line (start 6.604 0.127) (end 6.096 0.127) (layer F.SilkS) (width 0.2032))
  (fp_line (start -1.27 0.127) (end -1.016 0.127) (layer F.SilkS) (width 0.2032))
  (fp_line (start -1.27 0.127) (end -1.27 -0.8636) (layer F.SilkS) (width 0.2032))
  (fp_line (start -1.27 -0.8636) (end -0.9906 -1.143) (layer F.SilkS) (width 0.2032))
  (fp_line (start -1.27 0.127) (end -1.27 1.1176) (layer F.SilkS) (width 0.2032))
  (fp_line (start -1.27 1.1176) (end -0.9906 1.397) (layer F.SilkS) (width 0.2032))
  (fp_line (start 8.89 0.127) (end 8.636 0.127) (layer F.SilkS) (width 0.2032))
  (fp_line (start 8.89 0.127) (end 8.89 1.1176) (layer F.SilkS) (width 0.2032))
  (fp_line (start 8.89 1.1176) (end 8.6106 1.397) (layer F.SilkS) (width 0.2032))
  (fp_line (start 8.89 0.127) (end 8.89 -0.8636) (layer F.SilkS) (width 0.2032))
  (fp_line (start 8.89 -0.8636) (end 8.6106 -1.143) (layer F.SilkS) (width 0.2032))
  (pad 1 thru_hole oval (at 0 0 180) (size 1.524 3.048) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 2 thru_hole oval (at 2.54 0.254 180) (size 1.524 3.048) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 3 thru_hole oval (at 5.08 0 180) (size 1.524 3.048) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 4 thru_hole oval (at 7.62 0.254 180) (size 1.524 3.048) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
