(module CPOL-RADIAL-5MM-10MM-KIT (layer F.Cu) (tedit 200000)
  (descr "5 MM SPACED PTHS, WITH 10 MM SILK RING AND NO EXPOSED COPPER ON TOP")
  (tags "5 MM SPACED PTHS, WITH 10 MM SILK RING AND NO EXPOSED COPPER ON TOP")
  (attr virtual)
  (fp_text reference >NAME (at 0 -5.5118) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 0 5.588) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_line (start 1.4986 0.99822) (end 3.49758 0.99822) (layer F.SilkS) (width 0.06604))
  (fp_line (start 3.49758 0.99822) (end 3.49758 -0.99822) (layer F.SilkS) (width 0.06604))
  (fp_line (start 1.4986 -0.99822) (end 3.49758 -0.99822) (layer F.SilkS) (width 0.06604))
  (fp_line (start 1.4986 0.99822) (end 1.4986 -0.99822) (layer F.SilkS) (width 0.06604))
  (fp_line (start -1.905 -2.54) (end -3.175 -2.54) (layer F.SilkS) (width 0.2032))
  (fp_line (start 3.00736 -2.54) (end 1.99136 -2.54) (layer F.SilkS) (width 0.2032))
  (fp_line (start 2.49936 -3.048) (end 2.49936 -2.032) (layer F.SilkS) (width 0.2032))
  (fp_circle (center 0 0) (end 0 -4.99872) (layer F.SilkS) (width 0.2032))
  (fp_circle (center -2.49936 0) (end -2.49936 -0.44704) (layer F.SilkS) (width 0))
  (fp_circle (center 2.49936 0) (end 2.49936 -0.44958) (layer F.SilkS) (width 0))
  (fp_circle (center -2.49936 0) (end -2.49936 -0.9779) (layer F.SilkS) (width 0))
  (pad + thru_hole rect (at 2.49936 0) (size 1.9304 1.9304) (drill 0.89916) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad - thru_hole circle (at -2.49936 0) (size 1.9304 1.9304) (drill 0.89916) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
