(module 1X08_LOCK_LONGPADS (layer F.Cu) (tedit 5963D6E4)
  (descr "PLATED THROUGH HOLE -8 PIN LOCKING FOOTPRINT WITH LONG PADS")
  (tags "PLATED THROUGH HOLE -8 PIN LOCKING FOOTPRINT WITH LONG PADS")
  (attr virtual)
  (fp_text reference >NAME (at 0 -2.413) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 0 2.159) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_line (start 1.524 0) (end 1.016 0) (layer F.SilkS) (width 0.2032))
  (fp_line (start 4.064 0) (end 3.556 0) (layer F.SilkS) (width 0.2032))
  (fp_line (start 6.604 0) (end 6.096 0) (layer F.SilkS) (width 0.2032))
  (fp_line (start 9.144 0) (end 8.636 0) (layer F.SilkS) (width 0.2032))
  (fp_line (start 11.684 0) (end 11.176 0) (layer F.SilkS) (width 0.2032))
  (fp_line (start -1.27 0) (end -1.016 0) (layer F.SilkS) (width 0.2032))
  (fp_line (start -1.27 0) (end -1.27 -0.9906) (layer F.SilkS) (width 0.2032))
  (fp_line (start -1.27 -0.9906) (end -0.9906 -1.27) (layer F.SilkS) (width 0.2032))
  (fp_line (start -1.27 0) (end -1.27 0.9906) (layer F.SilkS) (width 0.2032))
  (fp_line (start -1.27 0.9906) (end -0.9906 1.27) (layer F.SilkS) (width 0.2032))
  (fp_line (start 14.224 0) (end 13.716 0) (layer F.SilkS) (width 0.2032))
  (fp_line (start 16.764 0) (end 16.256 0) (layer F.SilkS) (width 0.2032))
  (fp_line (start 19.05 0) (end 19.05 0.9906) (layer F.SilkS) (width 0.2032))
  (fp_line (start 19.05 0.9906) (end 18.7706 1.27) (layer F.SilkS) (width 0.2032))
  (fp_line (start 19.05 0) (end 19.05 -0.9906) (layer F.SilkS) (width 0.2032))
  (fp_line (start 19.05 -0.9906) (end 18.7706 -1.27) (layer F.SilkS) (width 0.2032))
  (fp_line (start 19.05 0) (end 18.796 0) (layer F.SilkS) (width 0.2032))
  (pad 1 thru_hole oval (at 0 -0.127 180) (size 1.524 3.048) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 2 thru_hole oval (at 2.54 0.127 180) (size 1.524 3.048) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 3 thru_hole oval (at 5.08 -0.127 180) (size 1.524 3.048) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 4 thru_hole oval (at 7.62 0.127 180) (size 1.524 3.048) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 5 thru_hole oval (at 10.16 -0.127 180) (size 1.524 3.048) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 6 thru_hole oval (at 12.7 0.127 180) (size 1.524 3.048) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 7 thru_hole oval (at 15.24 -0.127 180) (size 1.524 3.048) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 8 thru_hole oval (at 17.78 0.127 180) (size 1.524 3.048) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
