EESchema-DOCLIB  Version 2.0
#
$CMP ACS712
D ACS712 Hall-effect-based isolated linear current sensor <a href="http://www.sparkfun.com/datasheets/BreakoutBoards/0712.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/8883">SparkFun Low Current Sensor Breakout - ACS712</a> (SEN-08883)</li></ul>
K PROD_ID:IC-08964
$ENDCMP
#
$CMP AD627SOIC
D Hall-effect-based isolated linear current sensor<br><br>PROTO: IC-13132<br>
K PROD_ID:IC-13132
$ENDCMP
#
$CMP AD8232
D AD8232 Single Lead Heart Rate Monitor IC <a href="https://cdn.sparkfun.com/datasheets/Sensors/Biometric/AD8232.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/12650">SparkFun Single Lead Heart Rate Monitor - AD8232</a> (SEN-12650)</li></ul>
K PROD_ID:IC-11886
$ENDCMP
#
$CMP ADMP401
D ADMP401 - Omnidirection Bottom-Port MEMS Microphone The ADMP401 is a high quality, low cost, low power analog output bottom-ported omnidirectional MEMS microphone. The ADMP401 consists of a MEMS microphone element, an impedance converter, and an output amplifier. The ADMP401 sensitivity specification makes it an excellent choice for both near field and far field applications. <a href="http://www.analog.com/media/en/technical-documentation/obsolete-data-sheets/ADMP401.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/9868">SparkFun MEMS Microphone Breakout - INMP401 (ADMP401)</a> (BOB-09868)</li><li><a href="https://www.sparkfun.com/products/10028">MEMS Microphone - INMP401 (ADMP401)</a> (COM-10028)</li></ul>
K PROD_ID:IC-09773
$ENDCMP
#
$CMP ADXL193
D Analog Devices ADXL193 - 250g Accelerometer w/ Analog Output The ADXL193 is a small (5 mm x 5 mm x 2 mm ceramic LCC package), low power (1.5 mA current at 5V), single axis high-g iMEMS  accelerometer designed to sense shock and vibration at g-ranges of  120g or  250g. Three models are available and include AD22282-A-R2 ( 120g) and AD22283-B-R2 ( 250g). These products are used in a variety of crash/impact detection applications which include automotive airbag crash detection systems as well as medical, industrial, and sports equipment. <a href="https://www.sparkfun.com/datasheets/Sensors/Accelerometer/ADXL193.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/9332">SparkFun Single Axis Accelerometer Breakout - ADXL193 (+/-250g)</a> (SEN-09332)</li></ul>
K PROD_ID:IC-09219
$ENDCMP
#
$CMP ADXL330
D Analog Devices ADXL330 3-Axis Analog Accelerometer The ADXL330 is a small, thin, low power, complete 3-axis accelerometer with signal conditioned voltage outputs, all on a single monolithic IC. The product measures acceleration with a minimum full-scale range of  3g. It can measure the static acceleration of gravity in tilt-sensing applications, as well as dynamic acceleration resulting from motion, shock, or vibration. <a href="https://www.sparkfun.com/datasheets/Components/ADXL330_0.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/retired/692">Triple Axis Accelerometer Breakout - ADXL330</a> (SEN-00692)</li></ul>
K PROD_ID:IC-08189
$ENDCMP
#
$CMP ADXL335
D Analog Devices ADXL335 3-Axis Analog Accelerometer The ADXL335 is a small, thin, low power, complete 3-axis accelerometer with signal conditioned voltage outputs. The product measures acceleration with a minimum full-scale range of  3 g. It can measure the static acceleration of gravity in tiltsensing applications, as well as dynamic acceleration resulting from motion, shock, or vibration. <a href="https://www.sparkfun.com/datasheets/Components/SMD/adxl335.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/9269">SparkFun Triple Axis Accelerometer Breakout - ADXL335</a> (SEN-09269)</li><li><a href="https://www.sparkfun.com/products/9265">Triple Axis Accelerometer - ADXL335</a> (SEN-09265)</li></ul>
K PROD_ID:IC-08942
$ENDCMP
#
$CMP ADXL337
D Analog Devices ADXL337 3-Axis Analog Accelerometer The ADXL337 is a small, thin, low power, complete 3-axis accelerometer with signal conditioned voltage outputs. The product measures acceleration with a minimum full-scale range of  3g. It can measure the static acceleration of gravity in tiltsensing applications, as well as dynamic acceleration resulting from motion, shock, or vibration. <a href="https://cdn.sparkfun.com/datasheets/Sensors/Accelerometers/ADXL337.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/12786">SparkFun Triple Axis Accelerometer Breakout - ADXL337</a> (SEN-12786)</li></ul>
K PROD_ID:IC-12011
$ENDCMP
#
$CMP ADXL345
D Analog Devices ADXL345 3-Axis SPI/I2C 2/4/8/16g Accelerometer The ADXL345 is a small, thin, low power, 3-axis accelerometer with high resolution (13-bit) measurement at up to  16g. Digital output data is formatted as 16-bit twos complement and is accessible through either a SPI (3- or 4-wire) or I2C digital interface. <a href="https://www.sparkfun.com/datasheets/Sensors/Accelerometer/ADXL345.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/9836">SparkFun Triple Axis Accelerometer Breakout - ADXL345</a> (SEN-09836)</li><li><a href="https://www.sparkfun.com/products/9045">Triple Axis Accelerometer - ADXL345</a> (SEN-09045)</li><li><a href="https://www.sparkfun.com/products/10121">SparkFun 6 Degrees of Freedom IMU Digital Combo Board - ITG3200/ADXL345</a> (SEN-10121)</li></ul>
K PROD_ID:IC-09097
$ENDCMP
#
$CMP ADXL362
D Analog Devices ADXL362 3-Axis SPI Accelerometer The ADXL362 is an ultralow power, 3-axis MEMS accelerometer that consumes less than 2  A at a 100 Hz output data rate and 270 nA when in motion triggered wake-up mode. Unlike accelerometers that use power duty cycling to achieve low power consumption, the ADXL362 does not alias input signals by undersampling; it samples the full bandwidth of the sensor at all data rates. <a href="http://cdn.sparkfun.com/datasheets/BreakoutBoards/ADXL362.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/11446">SparkFun Triple Axis Accelerometer Breakout - ADXL362</a> (SEN-11446)</li></ul>
K PROD_ID:IC-11297
$ENDCMP
#
$CMP ADXL377
D Analog Devices ADXL377 Low Power 3-Axis  200 g Accelerometer with Analog Output The ADXL377 is a small, thin, low power, complete 3-axis accelerometer with signal conditioned voltage outputs. The ADXL377 measures acceleration resulting from motion, shock, or vibration with a typical full-scale range of  200g. <a href="https://cdn.sparkfun.com/datasheets/Sensors/Accelerometers/ADXL377.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/12803">SparkFun Triple Axis Accelerometer Breakout - ADXL377</a> (SEN-12803)</li></ul>
K PROD_ID:IC-12027
$ENDCMP
#
$CMP AK9750
D AK9750 Human Movement Sensor
K PROD_ID:SEN-13737
$ENDCMP
#
$CMP APDS-9960
D Avago APDS-9960 Digital Proximity, Ambient Light, RGB, and Gesture Sensor. The APDS-9960 offers ambient light and color measuring, proximity detection, and touchless gesture sensing. It features UV and IR blocking filters, four separate diodes sensitive to different directions, and an I2C compatible interface. <a href="https://cdn.sparkfun.com/datasheets/Sensors/Proximity/apds9960.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/12787">SparkFun RGB and Gesture Sensor - APDS-9960</a> (SEN-12787)</li></ul>
K PROD_ID:SEN-12005
$ENDCMP
#
$CMP AT42QT1012-TSHR
D Atmel AT42QT1010 1-Channel Capacitive Touch Sensor The AT42QT1010 is a dedicated, single-button capacitive sense chip. The chip handles monitoring a conductive area for touch. As long as a touch (e.g. from a finger) is detected, the AT42QT1010 keeps the output line high. Otherwise, the line is kept low. <a href="http://cdn.sparkfun.com/datasheets/Sensors/Capacitive/AT42QT1010_Datasheet.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/12041">SparkFun Capacitive Touch Breakout - AT42QT1010</a> (SEN-12041)</li></ul>
K PROD_ID:IC-11778
$ENDCMP
#
$CMP BME280
D Bosch BME280 &ndash; Combined Humidity and Pressure Sensor The  BME280 is as combined digital humidity, pressure and temperature sensor based on proven sensing principles. The sensor module is housed in an extremely compact metal-lid LGA package  with a footprint of only 2.5 2.5mm  with a height of 0.93mm. Its small dimensions and its low power consumption allow the implementation in battery driven devices such as handsets,  GPS modules or watches. <a href=https://cdn.sparkfun.com/assets/learn_tutorials/4/1/9/BST-BME280_DS001-10.pdf>Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/13676">SparkFun Atmospheric Sensor Breakout - BME280</a> (SEN-13676)</li></ul>
K PROD_ID:IC-13090
$ENDCMP
#
$CMP BMP180
D Bosch BMP180 Digital Barometric Pressures Sensor The BMP180 is the function compatible successor of the BMP085, a new generation of high precision digital pressure sensors for consumer applications. The ultra-low power, low voltage electronics of the BMP180 is optimized for use in mobile phones, PDAs, GPS navigation devices and outdoor equipment. With a low altitude noise of merely 0.25m at fast conversion time, the BMP180 offers superior performance. The I2C interface allows for easy system integration with a microcontroller. The BMP180 is based on piezo-resistive technology for EMC robustness, high accuracy and linearity as well as long term stability. Web page: <a href="http://www.bosch-sensortec.com/en/homepage/products_3/environmental_sensors_1/bmp180_1/bmp180">http://www.bosch-sensortec.com/en/homepage/products_3/environmental_sensors_1/bmp180_1/bmp180</a><br>Datasheet: <a href="http://ae-bst.resource.bosch.com/media/products/dokumente/bmp180/BST-BMP180-DS000-09.pdf"> http://ae-bst.resource.bosch.com/media/products/dokumente/bmp180/BST-BMP180-DS000-09.pdf</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/11823">Barometric Pressure Sensor - BMP180</a> (COM-11823)</li><li><a href="https://www.sparkfun.com/products/11824">SparkFun Barometric Pressure Sensor Breakout - BMP180</a> (SEN-11824)</li></ul>
K PROD_ID:IC-11600
$ENDCMP
#
$CMP BPW34
D Vishay BPW34 Silicon PIN Photodiode (Miniature Solar Cell) BPW34 is a PIN photodiode with high speed and high radiant sensitivity in miniature, flat, top view, clear plastic package. It is sensitive to visible and near infrared radiation. BPW34S is packed in tubes, specifications like BPW34. Datasheet: <a href="https://www.sparkfun.com/datasheets/Prototyping/Solar/bpw34.pdf">https://www.sparkfun.com/datasheets/Prototyping/Solar/bpw34.pdf</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/9541">Miniature Solar Cell - BPW34</a> (PRT-09541)</li></ul>
K PROD_ID:PRT-09541
$ENDCMP
#
$CMP BRM-2508RA
D BRM-2508 IR Receiver Module  2.7V/5.5V IR Receiver with Low Power Consumption, High-immunity Against Ambient Light. <a href="http://www.sinoskysun.com/upload/20110512/201105120447164615.PDF">Example Datasheet</a> 
K PROD_ID:COMP-12059
$ENDCMP
#
$CMP BRM-2508VERT
D BRM-2508 IR Receiver Module  2.7V/5.5V IR Receiver with Low Power Consumption, High-immunity Against Ambient Light. <a href="http://www.sinoskysun.com/upload/20110512/201105120447164615.PDF">Example Datasheet</a> 
K PROD_ID:COMP-12059
$ENDCMP
#
$CMP BRM-2A18RA
D BRM-2A18 IR Receiver The BRM-2A18 is miniaturized infrared receiver for remote control and other applications requiring improved ambient light rejection.  Vertical package is a primary component on the ZX Distance and Gesture Sensor. RA package is not currently in-use. <a href="http://www.sinoskysun.com/upload/20110512/201105120447164615.PDF">Example Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/12780">ZX Distance and Gesture Sensor</a> (COM-12780)</li></ul>
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP BRM-2A18VERT
D BRM-2A18 IR Receiver The BRM-2A18 is miniaturized infrared receiver for remote control and other applications requiring improved ambient light rejection.  Vertical package is a primary component on the ZX Distance and Gesture Sensor. RA package is not currently in-use. <a href="http://www.sinoskysun.com/upload/20110512/201105120447164615.PDF">Example Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/12780">ZX Distance and Gesture Sensor</a> (COM-12780)</li></ul>
K PROD_ID:COMP-12505
$ENDCMP
#
$CMP CCS811PRODUCTION
D AMS CCS811 &ndash; I<sup>2</sup>C Digital Gas Sensor Ultra-Low Power Digital Gas Sensor for Monitoring Indoor Air Quality <a href=http://ams.com/eng/Products/Environmental-Sensors/Gas-Sensors/CCS811>AMS Product Page</a> <b>SparkFun Products:</b><ul><li></li></ul> 
K PROD_ID:IC-13607
$ENDCMP
#
$CMP CCS811SKINNY
D AMS CCS811 &ndash; I<sup>2</sup>C Digital Gas Sensor Ultra-Low Power Digital Gas Sensor for Monitoring Indoor Air Quality <a href=http://ams.com/eng/Products/Environmental-Sensors/Gas-Sensors/CCS811>AMS Product Page</a> <b>SparkFun Products:</b><ul><li></li></ul> 
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP DS18B20
D Dallas/Maxim DS18B20 1-Wire Temperature Sensor The DS18B20 reports degrees C with 9 to 12-bit precision, -55C to 125C (+/-0.5C). Each sensor has a unique 64-Bit Serial number etched into it - allows for a huge number of sensors to be used on one data bus. <a href="http://datasheets.maximintegrated.com/en/ds/DS18B20.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/245">One Wire Digital Temperature Sensor - DS18B20</a> (SEN-00245)</li></ul>
K PROD_ID:SEN-00245
$ENDCMP
#
$CMP GAS_SENSORMQ-3
D Gas Sensors - MQ-3, MQ-4, MQ-6, MQ-7, MQ-8 Through-hole gas sensors with a heating coil and an analog output. <a href="https://cdn.sparkfun.com/datasheets/Sensors/Biometric/MQ-3%20ver1.3%20-%20Manual.pdf">Example Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/8891">Gas Sensor Breakout Board</a> (BOB-8891) - Breakout board compatible with all gas sensors.</li><li><a href="https://www.sparkfun.com/products/8880">Alcohol Gas Sensor - MQ-3</a> (SEN-08880)</li><li><a href="https://www.sparkfun.com/products/9404">Methane CNG Gas Sensor - MQ-4</a> (SEN-09404)</li><li><a href="https://www.sparkfun.com/products/9405">LPG Gas Sensor - MQ-6</a> (SEN-09405)</li><li><a href="https://www.sparkfun.com/products/9403">Carbon Monoxide Sensor - MQ-7</a> (SEN-09403)</li><li><a href="https://www.sparkfun.com/products/10916">Hydrogen Gas Sensor - MQ-8</a> (SEN-10916)</li></ul>
K PROD_ID:COMP-12216
$ENDCMP
#
$CMP GAS_SENSORMQ-4
D Gas Sensors - MQ-3, MQ-4, MQ-6, MQ-7, MQ-8 Through-hole gas sensors with a heating coil and an analog output. <a href="https://cdn.sparkfun.com/datasheets/Sensors/Biometric/MQ-3%20ver1.3%20-%20Manual.pdf">Example Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/8891">Gas Sensor Breakout Board</a> (BOB-8891) - Breakout board compatible with all gas sensors.</li><li><a href="https://www.sparkfun.com/products/8880">Alcohol Gas Sensor - MQ-3</a> (SEN-08880)</li><li><a href="https://www.sparkfun.com/products/9404">Methane CNG Gas Sensor - MQ-4</a> (SEN-09404)</li><li><a href="https://www.sparkfun.com/products/9405">LPG Gas Sensor - MQ-6</a> (SEN-09405)</li><li><a href="https://www.sparkfun.com/products/9403">Carbon Monoxide Sensor - MQ-7</a> (SEN-09403)</li><li><a href="https://www.sparkfun.com/products/10916">Hydrogen Gas Sensor - MQ-8</a> (SEN-10916)</li></ul>
K PROD_ID:COMP-11559
$ENDCMP
#
$CMP GAS_SENSORMQ-6
D Gas Sensors - MQ-3, MQ-4, MQ-6, MQ-7, MQ-8 Through-hole gas sensors with a heating coil and an analog output. <a href="https://cdn.sparkfun.com/datasheets/Sensors/Biometric/MQ-3%20ver1.3%20-%20Manual.pdf">Example Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/8891">Gas Sensor Breakout Board</a> (BOB-8891) - Breakout board compatible with all gas sensors.</li><li><a href="https://www.sparkfun.com/products/8880">Alcohol Gas Sensor - MQ-3</a> (SEN-08880)</li><li><a href="https://www.sparkfun.com/products/9404">Methane CNG Gas Sensor - MQ-4</a> (SEN-09404)</li><li><a href="https://www.sparkfun.com/products/9405">LPG Gas Sensor - MQ-6</a> (SEN-09405)</li><li><a href="https://www.sparkfun.com/products/9403">Carbon Monoxide Sensor - MQ-7</a> (SEN-09403)</li><li><a href="https://www.sparkfun.com/products/10916">Hydrogen Gas Sensor - MQ-8</a> (SEN-10916)</li></ul>
K PROD_ID:SEN-09405
$ENDCMP
#
$CMP GAS_SENSORMQ-7
D Gas Sensors - MQ-3, MQ-4, MQ-6, MQ-7, MQ-8 Through-hole gas sensors with a heating coil and an analog output. <a href="https://cdn.sparkfun.com/datasheets/Sensors/Biometric/MQ-3%20ver1.3%20-%20Manual.pdf">Example Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/8891">Gas Sensor Breakout Board</a> (BOB-8891) - Breakout board compatible with all gas sensors.</li><li><a href="https://www.sparkfun.com/products/8880">Alcohol Gas Sensor - MQ-3</a> (SEN-08880)</li><li><a href="https://www.sparkfun.com/products/9404">Methane CNG Gas Sensor - MQ-4</a> (SEN-09404)</li><li><a href="https://www.sparkfun.com/products/9405">LPG Gas Sensor - MQ-6</a> (SEN-09405)</li><li><a href="https://www.sparkfun.com/products/9403">Carbon Monoxide Sensor - MQ-7</a> (SEN-09403)</li><li><a href="https://www.sparkfun.com/products/10916">Hydrogen Gas Sensor - MQ-8</a> (SEN-10916)</li></ul>
K PROD_ID:COMP-12214
$ENDCMP
#
$CMP GAS_SENSORMQ-8
D Gas Sensors - MQ-3, MQ-4, MQ-6, MQ-7, MQ-8 Through-hole gas sensors with a heating coil and an analog output. <a href="https://cdn.sparkfun.com/datasheets/Sensors/Biometric/MQ-3%20ver1.3%20-%20Manual.pdf">Example Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/8891">Gas Sensor Breakout Board</a> (BOB-8891) - Breakout board compatible with all gas sensors.</li><li><a href="https://www.sparkfun.com/products/8880">Alcohol Gas Sensor - MQ-3</a> (SEN-08880)</li><li><a href="https://www.sparkfun.com/products/9404">Methane CNG Gas Sensor - MQ-4</a> (SEN-09404)</li><li><a href="https://www.sparkfun.com/products/9405">LPG Gas Sensor - MQ-6</a> (SEN-09405)</li><li><a href="https://www.sparkfun.com/products/9403">Carbon Monoxide Sensor - MQ-7</a> (SEN-09403)</li><li><a href="https://www.sparkfun.com/products/10916">Hydrogen Gas Sensor - MQ-8</a> (SEN-10916)</li></ul>
K PROD_ID:COMP-13351
$ENDCMP
#
$CMP GEIGER_TUBELND712
D LND, INC LND712 Geiger Tube Geiger tubes are the sensing elements of Geiger counters, which are used to measure ionizing radiation. This tube is made of a thin-walled stainless steel and is filled with a mixture of Neon and Halogen gases at low-pressure. <a href="http://www.sparkfun.com/datasheets/Components/General/LND-712-Geiger-Tube.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/8875">Geiger Tube</a> (COM-08875)</li><li><a href="https://www.sparkfun.com/products/11345">SparkFun Geiger Counter</a> (SEN-11345)</li></ul>
K PROD_ID:COMP-09328
$ENDCMP
#
$CMP GP1A57HR
D Sharp GP1A57HR Transmissive Photointerrupter Standard, OPIC output, transmissive photointerrupter with opposing emitter and detector in a case, providing non-contact sensing. 10mm gap. Built in 15k  pull-up resistor. <a href="https://www.sparkfun.com/datasheets/Components/GP1A57HRJ00F.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/9299">Photo Interrupter - GP1A57HRJ00F</a> (SEN-09299)</li><li><a href="https://www.sparkfun.com/products/9322">SparkFun Photo Interrupter Breakout Board - GP1A57HRJ00F</a> (BOB-09322) - Breakout board for above.</li></ul>
K PROD_ID:SEN-09299
$ENDCMP
#
$CMP HALL-EFFECT
D Panasonic AN4884 Hall Effect Sensor The AN48841B is a Hall IC (a magnetic sensor) for 3.0 V supply voltage built using Bi-CMOS technology. In this Hall IC are a Hall element, an offset cancel circuit, an amplifier circuit, a sample-and-hold circuit, a Schmidt circuit, and an output stage FET are integrated on a single chip housed in a small SC70 package. <a href="http://www.semicon.panasonic.co.jp/ds4/AN48841B_E.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/13169">SparkFun Blackberry Trackballer Breakout</a> (COM-13169) - Hall sensor is triggered by tiny magnets on trackball.</li></ul>
K PROD_ID:IC-09214
$ENDCMP
#
$CMP HIH-4030
D Honeywell HIH-4030 Humidity Sensor - Analog Output The HIH-4030/4031 Series delivers instrumentation-quality RH (Relative Humidity) sensing performance in a competitively priced, solderable SMD. <a href="https://www.sparkfun.com/datasheets/Sensors/Weather/SEN-09569-HIH-4030-datasheet.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/9569">SparkFun Humidity Sensor Breakout - HIH-4030</a> (SEN-09569)</li></ul>
K PROD_ID:IC-09448
$ENDCMP
#
$CMP HMC5883L
D Honewell HMC5883L 3 Axis Digital Compass IC a 3-axis digital magnetometer designed for low-field magnetic sensing. The sensor has a full-scale range of  8 Guass and a resolution of up to 5 milli-Gauss. Supplied voltage should be between 2.16 and 3.6VDC. Communication with the HMC5883L is simple and all done through an I2C interface. All registers and operating modes are well described in the datasheet below. <a href="http://cdn.sparkfun.com/datasheets/Sensors/Magneto/HMC5883L-FDS.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/10494">Magnetometer Digital Triple Axis - HMC5883L</a> (COM-10494)</li><li><a href="https://www.sparkfun.com/products/10530">SparkFun Triple Axis Magnetometer Breakout - HMC5883L</a> (SEN-10530)</li><li><a href="https://www.sparkfun.com/products/10736">9 Degrees of Freedom - Razor IMU</a> (SEN-10736)</li><li><a href="https://www.sparkfun.com/products/10724">SparkFun 9 Degrees of Freedom - Sensor Stick</a> (SEN-10724)</li></ul>
K PROD_ID:IC-10284
$ENDCMP
#
$CMP HMC6343
D Honewell HMC6343 Compass w/ Tilt Compensation The Honeywell HMC6343 is a fully integrated compass module that includes firmware  for  heading  computation and  calibration  for  magnetic  distortions.  The module combines three-axis magneto-resistive sensor, three-axis MEMS accelerometer,   analog   and   digital   support   circuits,   microprocessor and algorithms required for  heading  computation <a href="http://www51.honeywell.com/aero/common/documents/myaerospacecatalog-documents/Missiles-Munitions/HMC6343.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/12916">SparkFun HMC6343 Breakout </a> (SEN-12916)</li></ul>
K PROD_ID:IC-12117
$ENDCMP
#
$CMP HTU21D
D Measurement Specialties HTU21D Relative Humidity Sensor w/ Temperature HTU21D(F) digital humidity sensors are dedicated humidity and temperature plug and play transducers for OEM applications  where  reliable  and  accurate  measurements  are  needed.  Direct  interface  with  a  micro-controller  is made  possible  with  the  module for humidity  and  temperature  digital  outputs. These  low  power sensors are designed for high volume and cost sensitive applications with tight space constraints.  <a href="http://cdn.sparkfun.com/datasheets/BreakoutBoards/HTU21D.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/12064">SparkFun Humidity and Temperature Sensor Breakout - HTU21D</a> (SEN-12064)</li><li><a href="https://www.sparkfun.com/products/12081">SparkFun Weather Shield</a> (SEN-12081)</li><li><a href="https://www.sparkfun.com/products/13630">SparkFun Photon Weather Shield</a> (SEN-13630)</li></ul>
K PROD_ID:IC-11793
$ENDCMP
#
$CMP IDG1215
D Invensense IDG1215 Dual-Axis 67 &deg;/s Gyro he IDG-1215 is an integrated dual-axis angular rate sensor (gyroscope). It uses InvenSense s proprietary and patented MEMS technology with vertically driven, vibrating masses to make a functionally complete, low-cost, dual-axis angular rate sensor. All required electronics are integrated onto a single chip with the sensor. <a href="http://www.sparkfun.com/datasheets/Components/SMD/Datasheet_IDG1215.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/9071">Dual Axis Gyro - IDG1215</a> (COM-09071)</li><li><a href="https://www.sparkfun.com/products/9093">Gyro Breakout Board - IDG1215 Dual 67 /s</a> (SEN-09093)</li></ul>
K PROD_ID:IC-09061
$ENDCMP
#
$CMP ISL29125
D Intersil ISL29125 RGB Color Light Sensor The ISL29125 is a low power, high sensitivity, RED, GREEN and BLUE color light sensor (RGB) with an I2C (SMBus compatible) interface. Its state-of-the-art photodiode array provides an accurate RGB spectral response and excellent light source to light source variation (LS2LS). <a href="https://cdn.sparkfun.com/datasheets/Sensors/LightImaging/isl29125.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/12829">SparkFun RGB Light Sensor - ISL29125</a> (SEN-12829)</li></ul>
K PROD_ID:IC-12055
$ENDCMP
#
$CMP ITG-3200
D Invensense ITG-3200 3-Axis Gyroscope The ITG-3200 is the world s first single-chip, digital-output, 3-axis MEMS motion processing gyro optimized for gaming, 3D mice, and motion-based remote control applications for Internet connected Digital TVs and Set Top Boxes. The ITG-3200 features three 16-bit analog-to-digital converters (ADCs) for digitizing the gyro outputs, a user-selectable internal low-pass filter bandwidth, and a Fast-Mode I C (400kHz) interface. Additional features include an embedded temperature sensor and a 2% accurate internal oscillator. This breakthrough in MEMS motion processing gyro technology provides a dramatic 60% package size reduction, delivers a 60% power reduction, and has inherent cost advantages compared to competing multi-chip gyro solutions. <a href="https://www.sparkfun.com/datasheets/Sensors/Gyro/PS-ITG-3200-00-01.4.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/9793">Triple-Axis Digital-Output Gyroscope - ITG-3200</a> (SEN-09793)</li><li><a href="https://www.sparkfun.com/products/11977">SparkFun Triple-Axis Digital-Output Gyro Breakout - ITG-3200</a> (SEN-11977)</li><li><a href="https://www.sparkfun.com/products/10724">SparkFun 9 Degrees of Freedom - Sensor Stick</a> (SEN-10724)</li><li><a href="https://www.sparkfun.com/products/10121">SparkFun 6 Degrees of Freedom IMU Digital Combo Board - ITG3200/ADXL345</a> (SEN-10121)</li><li><a href="https://www.sparkfun.com/products/10736">9 Degrees of Freedom - Razor IMU</a> (SEN-10736)</li></ul>
K PROD_ID:IC-09685
$ENDCMP
#
$CMP L3G4200D
D ST Microelectronics L3G4200D 3-Axis Digital Output Gyroscope The L3G4200D is a low-power three-axis angular rate sensor, has a full scale of  250/ 500/ 2000 dps and is capable of measuring rates with a user-selectable bandwidth.<br><br>It includes a sensing element and an IC interface capable of providing the measured angular rate to the external world through a digital interface (I2C/SPI). <a href="http://cdn.sparkfun.com/datasheets/Sensors/Gyros/3-Axis/CD00265057.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/10612">SparkFun Tri-Axis Gyro Breakout - L3G4200D</a> (SEN-10612)</li></ul>
K PROD_ID:IC-10395
$ENDCMP
#
$CMP LIGHT_SENSORALS
D Ambient Light Sensors - Phototransistors Low cost ambient light sensors, consisting of a phototransistor in miniature SMD packages. Output voltage varies with light intensity. <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/12566">ALS-PT19 Light Sensor</a> (SEN-12566)</li><li><a href="https://www.sparkfun.com/products/8348">Ambient Light Sensor - TEMT6000</a> (SEN-08348)</li><li><a href="https://www.sparkfun.com/products/8688">SparkFun Ambient Light Sensor Breakout - TEMT60000</a> (SEN-08688)</li></ul>
K PROD_ID:IC-11836
$ENDCMP
#
$CMP LIGHT_SENSORTEMT6000
D Ambient Light Sensors - Phototransistors Low cost ambient light sensors, consisting of a phototransistor in miniature SMD packages. Output voltage varies with light intensity. <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/12566">ALS-PT19 Light Sensor</a> (SEN-12566)</li><li><a href="https://www.sparkfun.com/products/8348">Ambient Light Sensor - TEMT6000</a> (SEN-08348)</li><li><a href="https://www.sparkfun.com/products/8688">SparkFun Ambient Light Sensor Breakout - TEMT60000</a> (SEN-08688)</li></ul>
K PROD_ID:COMP-08569
$ENDCMP
#
$CMP LIS331
D ST Microelectronics LIS331 3-Axis &plusmn;6/12/24g SPI/I2C Accelerometer The LIS331HH is an ultra low-power full-scale three axis MEMS linear accelerometer. It has a digital I2C/SPI serial interface which makes it ideal for using in embedded applications. The device also features ultra low-power operational modes that allow advanced power saving and smart sleep to wake-up functions. <a href="http://www.sparkfun.com/datasheets/Sensors/Accelerometer/LIS331HH.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/10345">SparkFun Triple Axis Accelerometer Breakout - LIS331</a> (SEN-10345)</li><li><a href="https://www.sparkfun.com/products/9755">Triple Axis Accelerometer - LIS331HH</a> (SEN-09755)</li></ul>
K PROD_ID:IC-12675
$ENDCMP
#
$CMP LIS3DH
D ST Microelectronics LIS3DH 3-Axis &plusmn;2/4/8/16g SPI/I2C Accelerometer The LIS3DH is a three axis MEMS linear accelerometer in the "nano" family. It has a digital I2C/SPI serial interface which makes it ideal for using in embedded applications. The device also features ultra low-power operational modes that allow advanced power saving and smart sleep to wake-up functions, built in detections with interrupts, and auxiliary ADC inputs <a href="http://www.sparkfun.com/datasheets/Sensors/Accelerometer/LIS3DH.pdf">Datasheet-XXXX</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/10345">SparkFun Triple Axis Accelerometer Breakout - LIS3DH</a> (SEN-XXXXX)</li><li><a href="https://www.sparkfun.com/products/9755">Triple Axis Accelerometer - LIS3DH</a> (SEN-XXXXX)</li></ul>
K PROD_ID:IC-13419
$ENDCMP
#
$CMP LM34DM
D Texas Instruments LM34 - Precision Fahrenheit Temperature Sensor 10mV/degF, 1 degF accurate analog temp sensor <a href="http://www.ti.com/lit/ds/symlink/lm34.pdf">Datasheet</a> 
K PROD_ID:IC-08232
$ENDCMP
#
$CMP LOAD_CELL1X03-PTH
D Load Cell - Half-Wheatstone Bridge Load cell weight sensors commonly found in scales. 3- pin, half-wheatstone bridge configuration. <a href="http://www.sparkfun.com/datasheets/Sensors/loadsensor.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/10245">Load Sensor - 50kg</a> (SEN-10245)</li></ul>
K PROD_ID:SEN-10245
$ENDCMP
#
$CMP LSM303C
D Ultra-compact high-performance eCompass module 3D accelerometer and 3D magnetometer  <a href="http://www.st.com/web/en/resource/technical/document/datasheet/DM00089896.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/13303">SparkFun 6 Degrees of Freedom Breakout - LSM303C</a> (BOB-13303)</li></ul>
K PROD_ID:IC-12557
$ENDCMP
#
$CMP LSM9DS0
D LSM9DS0 3D Accelerometer, 3D Gyroscope, 3D Magnetomter Replaced by LSM9DS1 <h4>Features:</h4><ul><li>3 acceleration channels, 3 angular rate</li>channels, 3 magnetic field channels</li><li> 2/ 4/ 6/ 8/ 16 g linear acceleration full scale</li><li> 2/ 4/ 8/ 12 gauss magnetic full scale</li><li>  245/ 500/ 2000 dps angular rate full scale</li><li> 16-bit data output</li><li> SPI / I2C serial interfaces</li><li> Analog supply voltage 2.4 V to 3.6 V</li><li> Power-down mode / low-power mode</li><li> Programmable interrupt generators</li><li> Embedded self-test</li><li> Embedded temperature sensor</li><li> Embedded FIFO</li><li> Position and motion detection functions</li><li> Click/double-click recognition</li></ul> <a href="">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/13033">SparkFun Block for Intel  Edison - 9 Degrees of Freedom</a> (DEV-13033)</li></ul>
K PROD_ID:IC-11867
$ENDCMP
#
$CMP LSM9DS1
D ST Microelectronics LSM9DS1 9DOF IMU - Accelerometer, Gyroscope & Magnetometer The LSM9DS1 is a versatile, motion-sensing system-in-a-chip. It houses a 3-axis accelerometer, 3-axis gyroscope, and 3-axis magnetometer   nine degrees of freedom (9DOF) in a single IC! The LSM9DS1 is equipped with a digital interface, but even that is flexible: it supports both I2C and SPI, so you ll be hard-pressed to find a microcontroller it doesn t work with. <a href="https://cdn.sparkfun.com/assets/learn_tutorials/3/7/3/LSM9DS1_Datasheet.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/13284">SparkFun 9 Degrees of Freedom IMU Breakout - LSM9DS1</a> (SEN-13284)</li><li><a href="https://www.sparkfun.com/products/13629">SparkFun Photon IMU Shield</a> (DEV-13629)</li></ul>
K PROD_ID:IC-12536
$ENDCMP
#
$CMP LTR-301
D LiteOn LTR-301 IR Phototransistor (Side-Receiving) Side-looking Infrared detectors. These simple devices operate at 940nm and work well for generic IR systems including remote control and touch-less object sensing. Using a simple ADC on any microcontroller will allow variable readings to be collected from the detector. <a href="http://www.sparkfun.com/datasheets/Components/LTR-301.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/241">Infrared Emitters and Detectors</a> (SEN-00241)</li></ul>
K PROD_ID:DIO-10904
$ENDCMP
#
$CMP MAG3110
D Freescale MAG3110 3-Axis Digital (I2C) Magnetometer Freescale s MAG3110 is a small, low-power, digital 3-axis magnetometer. The device can be used in conjunction with a 3-axis accelerometer to produce orientation independent accurate compass heading information. It features a standard I2C serial interface output and smart embedded functions. <a href="https://cdn.sparkfun.com/datasheets/Sensors/Magneto/MAG3110_v9.2.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/12670">SparkFun Triple Axis Magnetometer Breakout - MAG3110</a> (SEN-12670)</li></ul>
K PROD_ID:IC-10404
$ENDCMP
#
$CMP MAX30105SMD
D MAX30105 High Sensitivity Optical Sensor Can be used for Pulse Detection, Pulse Ox, and possible visual particle detection. </br>I2C communication.<li><a href= https://datasheets.maximintegrated.com/en/ds/MAX30105.pdf >Datasheet</a></li> <b>SparkFun Products:</b><ul><li><a href= https://www.sparkfun.com/products/14045 >SparkFun Particle Sensor Breakout - MAX30105</a></li></ul> 
K PROD_ID:IC-13510
$ENDCMP
#
$CMP MCP9700TT
D Microchip MCP9700 Analog-Output Temperature Sensor The MCP9700 can accurately measure temperature from -40C to +150C. The output of the MCP9700 is calibrated to a slope of 10mV/ C and has a DC offset of 500mV. The offset allows reading negative temperatures without the need for a negative supply.  <a href="http://ww1.microchip.com/downloads/en/DeviceDoc/20001942F.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/8777">LilyPad Temperature Sensor</a> (DEV-08777)</li><li><a href="https://www.sparkfun.com/products/12651">SparkFun Digital Sandbox</a> (DEV-12651)</li></ul>
K PROD_ID:IC-08917
$ENDCMP
#
$CMP MIC-PTH
D Microphone Omni-directional electret microphones - one through-hole, the other SMD. <a href="http://cdn.sparkfun.com/datasheets/Sensors/Sound/CEM-C9745JAD462P2.54R.pdf">Datasheet</a> (through-hole mic) <a href="http://www.challengeelectronics.com/downloads/microphones/omni_directional/CEM-OB6018-3EAD443C43MR.pdf">Datasheet</a> (SMD mic) <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/8635">PTH Electret Microphone</a> (COM-08635)</li><ul><li><a href="https://www.sparkfun.com/products/9964">SparkFun Electret Microphone Breakout </a> (BOB-09964)</li><li><a href="https://www.sparkfun.com/products/12651">Digital Sandbox</a> (DEV-12651)</li><li><a href="https://www.sparkfun.com/products/12642">SparkFun Sound Detector</a> (SEN-12642)</li></ul><li>SMD Microphone</li><ul><a href="https://www.sparkfun.com/products/retired/10653">SparkFun Voice Recorder Breakout - ISD1932</a> (BOB-10653)</li>
K PROD_ID:COMP-08856
$ENDCMP
#
$CMP ML8511
D Lapis ML8511 Ultraviolet Sensor The MP8511 UV (ultraviolet) Sensor works by outputing an analog signal in relation to the amount of UV light that s detected. This sensor detects 280-390nm light most effectively. This is categorized as part of the UVB (burning rays) spectrum and most of the UVA (tanning rays) spectrum. It outputs a analog voltage that is linearly related to the measured UV intensity (mW/cm2). <a href="https://cdn.sparkfun.com/datasheets/Sensors/LightImaging/ML8511_3-8-13.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/12705">SparkFun UV Sensor Breakout - ML8511 </a> (SEN-12705)</li></ul>
K PROD_ID:IC-11927
$ENDCMP
#
$CMP MLX90614
D Melexis MLX90614 Infrared (IR) Thermometer The MLX90614 is a passive infrared (PIR) I<sup>2</sup>C temperature sensor.It is designed for non-contact temperature sensing. An internal 17-bit ADC and a powerful DSP contribute to the MLX90614 s high accuracy and resolution. It has a huge number of applications including body temperature measurment and movement detection. <a href="http://www.sparkfun.com/datasheets/Sensors/Temperature/SEN-09570-datasheet-3901090614M005.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/9570">Infrared Thermometer - MLX90614</a> (SEN-09570)</li><li><a href="https://www.sparkfun.com/products/10740">SparkFun IR Thermometer Evaluation Board - MLX90614 </a> (SEN-10740)</li></ul>
K PROD_ID:COMP-09719
$ENDCMP
#
$CMP MMA8452Q
D NXP MMA8452Q 3-Axis Digital Accelerometer The MMA8452Q is a smart low-power, three-axis, capacitive MEMS accelerometer with 12 bits of resolution. This accelerometer is packed with embedded functions with flexible user programmable options, configurable to two interrupt pins.  <ul><li><B>Supply Voltage:</b> 1.6-3.6V</li><li><B>Range:</b> +/- 2g, 4g, 8g</li><li><B>Interface:</b> I<sup>2</sup>C, 12-bit and 8-bit</li><li><b>ODR:</b> 1.56 Hz - 800 Hz</li><li><B>Package:</b> QFN-16</li></ul><a href="http://cache.freescale.com/files/sensors/doc/data_sheet/MMA8452Q.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/12756">SparkFun Triple Axis Accelerometer Breakout - MMA8452Q</a> (SEN-12756)</li><li><a href="https://www.sparkfun.com/products/12589">SparkFun RedBot Sensor - Accelerometer</a> (SEN-12589)</li></ul>
K PROD_ID:IC-10769
$ENDCMP
#
$CMP MPL115A
D NXP MPL115A 50 to 115kPa, Absolute Digital Pressure Sensor The MPL115A is a simple barometer with digital output for cost-effective applications. It employs a MEMS pressure sensor with a conditioning integrated circuit to provide accurate pressure data. An integrated analog-to-digital converter (ADC) provides digitized temperature and pressure sensor outputs via either a serial peripheral interface (SPI) (MPL115A1) or I C (MPL115A2) port. <a href="http://www.sparkfun.com/datasheets/Sensors/Pressure/MPL115A1.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/9721">SparkFun Barometric Pressure Sensor Breakout - MPL115A1</a> (SEN-09721)</li><li><a href="https://www.sparkfun.com/products/9602">Barometric Pressure Sensor - MPL115A1</a> (SEN-09602)</li></ul>
K PROD_ID:IC-09492
$ENDCMP
#
$CMP MPL3115A2
D NXP MPL3115A2 Digital Altimeter/Pressure Sensor The MPL3115A2 is a compact piezoresistive absolute pressure sensor with an I2C interface. MPL3115 has a wide operating range of 20kPa to 110 kPa, a range that covers all surface elevations on Earth. The fully internally compensated MEMS in conjunction with an embedded high resolution 24-bit equivalent ADC provide accurate pressure [Pascals] /altitude [meters] and temperature [degrees Celsius] data. <a href="http://cdn.sparkfun.com/datasheets/Sensors/Pressure/MPL3115A2.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/11084">SparkFun Altitude/Pressure Sensor Breakout - MPL3115A2</a> (SEN-11084)</li><li><a href="https://www.sparkfun.com/products/12081">SparkFun Weather Shield</a> (DEV-12081)</li><li><a href="https://www.sparkfun.com/products/13630">SparkFun Photon Weather Shield</a> (DEV-13630)</li></ul>
K PROD_ID:IC-10869
$ENDCMP
#
$CMP MPR121
D NXP MPR121 Proximity Capacitive Touch Sensor Controller The MPR121 is a capacitive touch sensor controller driven by an I2C interface. The chip can control up to twelve individual electrodes, as well as a simulated thirteenth electrode. The MPR121 also features eight LED driving pins. When these pins are not configured as electrodes, they may be used to drive LEDs. <a href="http://www.sparkfun.com/datasheets/Components/MPR121.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/9604">Capacitive Touch Sensor Controller - MPR121QR2</a> (COM-09604)</li><li><a href="https://www.sparkfun.com/products/9695">SparkFun Capacitive Touch Sensor Breakout - MPR121</a> (SEN-09695)</li><li><a href="https://www.sparkfun.com/products/12013">SparkFun Touch Shield</a> (DEV-12013)</li><li><a href="https://www.sparkfun.com/products/12017">SparkFun Capacitive Touch Keypad - MPR121</a> (SEN-12017)</li></ul>
K PROD_ID:IC-09490
$ENDCMP
#
$CMP MPU-6000
D Invensense MPU-6000 6-Axis Gryoscope/Accelerometer 3-axis gyroscope, 3-axis accelerometer in a 4x4 package. The MPU-6000 is the world s first 6-axis I C MotionTracking device designed for the low power, low cost, and high performance requirements of smartphones, tablets and wearable sensors. <a href="http://cdn.sparkfun.com/datasheets/Components/General%20IC/PS-MPU-6000A.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/11234">MPU-6000 - Motion Processing Unit</a> (SEN-11234)</li><li><a href="https://www.sparkfun.com/products/11703">SparkFun UDB5 - PIC UAV Development Board</a> (GPS-11703)</li></ul>
K PROD_ID:IC-11089
$ENDCMP
#
$CMP MPU-9250
D MPU-9250 9 Degree of Freedom IMU  System in Package that contains MPU-6500 & AK8963 <br>NC pin 19. 2-6 & 14-17 not internally connected. May be used for PCB trace routing.<br><a href= https://cdn.sparkfun.com/assets/learn_tutorials/5/5/0/MPU9250REV1.0.pdf >Datasheet</a> <b>SparkFun Products:</b><ul><li><a href= https://www.sparkfun.com/products/14001 >SparkFun 9DoF Razor IMU M0</a></li><li><a href= https://www.sparkfun.com/products/13762 >SparkFun IMU Breakout - MPU-9250</a></li></ul> 
K PROD_ID:IC-13192
$ENDCMP
#
$CMP MS5803-14BA
D Measurement Specialties MS5803_14BA Pressure (Depth) Sensor The MS5803-14BA is a new generation of high resolution pressure sensors with SPI and I2C bus interface. It is optimized for depth measurement systems with a water depth resolution of 1cm and below. The sensor module includes a high linear pressure sensor and an ultra low power 24 bit    ADC with internal factory calibrated coefficients. It provides a precise digital 24 Bit pressure and temperature value and different operation modes that allow the user to optimize for conversion speed and current consumption. <a href="https://cdn.sparkfun.com/datasheets/Sensors/Weather/ms5803_14ba.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/12909">SparkFun Pressure Sensor Breakout - MS5803-14BA</a> (SEN-12909)</li></ul>
K PROD_ID:IC-12111
$ENDCMP
#
$CMP PHOTOCELLPTH
D Photocell (Photodetector, Photo Resistor, CdS) This is a very small light sensor. A photocell changes (also called a photodetector, photo resistor, CdS or photoconductive cell) resistance depending on the amount of light it is exposed to. These little sensors make great ambient light triggers (when light in the room turns on, do something). <a href="http://cdn.sparkfun.com/datasheets/Sensors/LightImaging/SEN-09088.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/9088">Mini Photocell</a> (SEN-09088)</li></ul>
K PROD_ID:COMP-09129
$ENDCMP
#
$CMP PHOTOCELLPTH-KIT
D Photocell (Photodetector, Photo Resistor, CdS) This is a very small light sensor. A photocell changes (also called a photodetector, photo resistor, CdS or photoconductive cell) resistance depending on the amount of light it is exposed to. These little sensors make great ambient light triggers (when light in the room turns on, do something). <a href="http://cdn.sparkfun.com/datasheets/Sensors/LightImaging/SEN-09088.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/9088">Mini Photocell</a> (SEN-09088)</li></ul>
K PROD_ID:COMP-09129
$ENDCMP
#
$CMP QRD1114
D QRD1114 Reflective Proximity, Object Sensor This sensor uses an infrared emitted diode combined with an infrared phototransistor to detect the reflected infrared signal. Ideal for sensing black-to-white transitions or can be used to detect nearby objects (.5-1cm). <a href="http://www.sparkfun.com/datasheets/BOT/QRD1114.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/246">Optical Detector / Phototransistor - QRD1114</a> (SEN-00246)</li></ul>
K PROD_ID:IC-09032
$ENDCMP
#
$CMP QRE1113
D QRE1113 Reflective Object Sensor The QRE1113 is a small IR reflectance sensor. This sensor is often used in line following robots because, if it can sense if a surface is white or black. There are four pins on the QRE1113 - two control the IR emitting LED while the other two are the collector and emitter of a phototransistor. The IR diode has a max forward current of 50mA and operates at 940nm. <a href="http://www.sparkfun.com/datasheets/Components/SMD/QRE1113.GR.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/9542">IR Reflectance Sensor - QRE1113</a> (COM-09542)</li><li><a href="https://www.sparkfun.com/products/9453">SparkFun Line Sensor Breakout - QRE1113 (Analog)</a> (ROB-09453)</li><li><a href="https://www.sparkfun.com/products/9454">SparkFun Line Sensor Breakout - QRE1113 (Digital)</a> (ROB-09454)</li><li><a href="https://www.sparkfun.com/products/11769">SparkFun RedBot Sensor - Line Follower</a> (SEN-11769)</li><li><a href="https://www.sparkfun.com/products/12617">SparkFun RedBot Sensor - Wheel Encoder</a> (SEN-12617)</li><li><a href="https://www.sparkfun.com/products/13582">SparkFun Line Follower Array</a> (SEN-13582)</li></ul>
K PROD_ID:IC-09357
$ENDCMP
#
$CMP QRE1113SMD-W
D QRE1113 Reflective Object Sensor The QRE1113 is a small IR reflectance sensor. This sensor is often used in line following robots because, if it can sense if a surface is white or black. There are four pins on the QRE1113 - two control the IR emitting LED while the other two are the collector and emitter of a phototransistor. The IR diode has a max forward current of 50mA and operates at 940nm. <a href="http://www.sparkfun.com/datasheets/Components/SMD/QRE1113.GR.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/9542">IR Reflectance Sensor - QRE1113</a> (COM-09542)</li><li><a href="https://www.sparkfun.com/products/9453">SparkFun Line Sensor Breakout - QRE1113 (Analog)</a> (ROB-09453)</li><li><a href="https://www.sparkfun.com/products/9454">SparkFun Line Sensor Breakout - QRE1113 (Digital)</a> (ROB-09454)</li><li><a href="https://www.sparkfun.com/products/11769">SparkFun RedBot Sensor - Line Follower</a> (SEN-11769)</li><li><a href="https://www.sparkfun.com/products/12617">SparkFun RedBot Sensor - Wheel Encoder</a> (SEN-12617)</li><li><a href="https://www.sparkfun.com/products/13582">SparkFun Line Follower Array</a> (SEN-13582)</li></ul>
K PROD_ID:IC-09357
$ENDCMP
#
$CMP SHT1XSHT15
D Sensiron SHT1x (SHT10, SHT11, SHT15) Digital Humidity Sensor The SHT1x humidity sensor series (including SHT10, SHT11, and SHT15) is Sensirion s family of surface-mountable relative humidity sensors. The humidity sensors integrate sensor elements plus signal processing on a tiny footprint and provide a fully calibrated digital output. A unique capacitive sensor element is used for measuring relative humidity, while temperature is measured by a band-gap sensor. <a href="https://cdn.sparkfun.com/datasheets/Sensors/Pressure/Sensirion_Humidity_SHT1x_Datasheet_V5.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/8227">Humidity and Temperature Sensor - SHT15</a> (COM-08227)</li><li><a href="https://www.sparkfun.com/products/13683">SparkFun Humidity and Temperature Sensor Breakout - SHT15</a> (SEN-13683)</li></ul>
K PROD_ID:IC-08303
$ENDCMP
#
$CMP SI7021
D Silicon Labs Si7021 I<sup>2</sup>C Humidity and Temperature Sensor The Si7021 is a low-cost, easy-to-use, highly accurate, digital humidity and temperature sensor. This sensor is ideal for environmental sensing and data logging and perfect for build a weather stations or humidor control system. All you need are two lines for I2C communication, and you ll have relative humidity readings and very accurate temperature readings as a bonus! <a href="https://cdn.sparkfun.com/datasheets/Sensors/Weather/Si7021.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/13763">SparkFun Humidity and Temperature Sensor Breakout - Si7021</a> (SEN-13763)</li><li><a href="https://www.sparkfun.com/products/13794">SparkFun Blynk Board - ESP8266</a> (WRL-13794)</li></ul>
K PROD_ID:IC-13093
$ENDCMP
#
$CMP SOLAR-IXYS
D IXYS CPC1822 4V Output Solar Cell The CPC1822 is a monolithic photovoltaic string of solar cells with switching circuitry. When operating in sunlight or a bright artificial light environment the optical energy will activate the cell array and generate a voltage at the output. The solar cells are capable of generating a floating source voltage and current sufficient to drive and power CMOS ICs, logic gates and/or provide  trickle charge  for battery applications. <a href="https://www.sparkfun.com/datasheets/Prototyping/Solar/CPC1822-1.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/9962">Miniature Solar Cell - CPC1822</a> (PRT-09962)</li></ul>
K PROD_ID:PRT-09962
$ENDCMP
#
$CMP T5403
D Epcos T5403 Digital Barometric Pressure Sensor The T5403 sensor measures the absolute pressure of the air around. This pressure varies with both the weather and altitude. Depending on how you interpret the data, you can monitor changes in the weather, measure altitude, or any other tasks that require an accurate pressure reading. <a href="http://cdn.sparkfun.com/datasheets/Sensors/Weather/T5400.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/12039">SparkFun Barometric Sensor Breakout - T5403</a> (SEN-12039)</li></ul>
K PROD_ID:IC-11772
$ENDCMP
#
$CMP TCM8240MD
D Toshiba TCM8240MD 1.3MP Color Image Sensor The TCM8240MD is a high quality, very small 1.3 mega-pixel color camera from Toshiba with the standard data+I2C interface. The nice thing is that we have a good supplier of these cameras, so they should be around for some time. This camera is also unique in that it offers on-board JPEG compression. <a href="http://www.sparkfun.com/datasheets/Sensors/Imaging/TCM8240MD_E150405_REV13.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/retired/8668">CMOS Camera - 1300x1040</a> (SEN-08668)</li><li><a href="https://www.sparkfun.com/products/retired/9504">TCM8240 Camera Breakout</a> (BOB-09504)</li></ul>
K PROD_ID:COMP-09354
$ENDCMP
#
$CMP TMP006
D Infrared Temperature Sensor TMP006 3.3v to 5.0v <a href="http://cdn.sparkfun.com/datasheets/Sensors/Temp/tmp006.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/11859">SparkFun Infrared Temperature Breakout - TMP006</a> (SEN-11859)</li></ul>
K PROD_ID:IC-11632
$ENDCMP
#
$CMP TMP102
D Texas Instruments TMP102 Low-Power Digital Temperature Sensor The TMP102 is a digital sensor (I2C a.k.a. TWI), has a resolution of 0.0625 C, and is accurate up to 0.5 C. This is a very handy sensor that requires a very low-current. <a href="http://www.sparkfun.com/datasheets/Sensors/Temperature/tmp102.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/11931">SparkFun Digital Temperature Sensor Breakout - TMP102</a> (SEN-11931)</li></ul>
K PROD_ID:IC-09303
$ENDCMP
#
$CMP TMP36GT9
D TMP36 Precision Analog &deg;C Temperature Sensor The TMP36 is a low voltage, precision centigrade temperature sensor. It provides a voltage output that is linearly proportional to the Celsius temperature. It also doesn t require any external calibration to provide typical accuracies of  1 C at +25 C and  2 C over the  40 C to +125 C temperature range. We like it because it s so easy to use: Just give the device a ground and 2.7 to 5.5 VDC and read the voltage on the Vout pin. The output voltage can be converted to temperature easily using the scale factor of 10 mV/ C. <a href="http://cdn.sparkfun.com/datasheets/Sensors/Temp/TMP35_36_37.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/10988">Temperature Sensor - TMP36</a> (SEN-10988)</li><li><a href="https://www.sparkfun.com/products/11649">SparkFun Danger Shield</a> (DEV-11649)</li></ul>
K PROD_ID:IC-09880
$ENDCMP
#
$CMP TMP36GT9-KIT
D TMP36 Precision Analog &deg;C Temperature Sensor The TMP36 is a low voltage, precision centigrade temperature sensor. It provides a voltage output that is linearly proportional to the Celsius temperature. It also doesn t require any external calibration to provide typical accuracies of  1 C at +25 C and  2 C over the  40 C to +125 C temperature range. We like it because it s so easy to use: Just give the device a ground and 2.7 to 5.5 VDC and read the voltage on the Vout pin. The output voltage can be converted to temperature easily using the scale factor of 10 mV/ C. <a href="http://cdn.sparkfun.com/datasheets/Sensors/Temp/TMP35_36_37.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/10988">Temperature Sensor - TMP36</a> (SEN-10988)</li><li><a href="https://www.sparkfun.com/products/11649">SparkFun Danger Shield</a> (DEV-11649)</li></ul>
K PROD_ID:IC-09880
$ENDCMP
#
$CMP TSL2561FN
D TAOS TSL2561 Digital Luminosity (Light) Sensor The TSL2561 is a light-to-digital converter that transform light intensity to a digital signal output via I2C interface. The device combines one broadband photodiode (visible plus infrared) and one infrared-responding photodiode on a single CMOS integrated circuit capable of providing a near-photopic response over an effective 20-bit dynamic range (16-bit resolution). Two integrating ADCs convert the photodiode currents to a digital output that represents the irradiance measured on each channel. This digital output can be input to a microprocessor where illuminance (ambient light level) in lux is derived using an empirical formula to approximate the human eye response. The TSL2561 device supports a traditional level style interrupt that remains asserted until the firmware clears it. <a href="http://www.mouser.com/ds/2/588/ams_sl2560-e58-488842.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/12055">SparkFun Luminosity Sensor Breakout - TSL2561</a> (SEN-12055)</li></ul>
K PROD_ID:IC-11791
$ENDCMP
#
$CMP TSL2561T
D TAOS TSL2561 Digital Luminosity (Light) Sensor The TSL2561 is a light-to-digital converter that transform light intensity to a digital signal output via I2C interface. The device combines one broadband photodiode (visible plus infrared) and one infrared-responding photodiode on a single CMOS integrated circuit capable of providing a near-photopic response over an effective 20-bit dynamic range (16-bit resolution). Two integrating ADCs convert the photodiode currents to a digital output that represents the irradiance measured on each channel. This digital output can be input to a microprocessor where illuminance (ambient light level) in lux is derived using an empirical formula to approximate the human eye response. The TSL2561 device supports a traditional level style interrupt that remains asserted until the firmware clears it. <a href="http://www.mouser.com/ds/2/588/ams_sl2560-e58-488842.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/12055">SparkFun Luminosity Sensor Breakout - TSL2561</a> (SEN-12055)</li></ul>
K PROD_ID:XXX-00000
$ENDCMP
#
$CMP TSOP57238TT1
D Vishay TSOP572...TT1 (TSOP57238TT1) IR Receiver Module The  TSOP57...  series  are  miniaturized  SMD  IR  receiver  modules  for  infrared  remote  control  systems.  A  PIN  diode  and  a  preamplifier  are  assembled  on  a  PCB,  the  epoxy  package contains an IR filter. The demodulated output signal can be directly connected to a microprocessor for decoding. <a href="http://www.vishay.com/docs/82434/tsop572.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li> Not currently in a SparkFun Assembly</ul>
K PROD_ID:COMP-11990
$ENDCMP
#
$CMP VL6180
D ST VL6180X Proximity and Ambient Light Sensing (ALS) Module  Instead of estimating the distance by measuring the amount of light reflected back from the object (which is significantly influenced by color and surface), the VL6180 precisely measures the time the light takes to travel to the nearest object and reflect back to the sensor (Time-of-Flight). Combining an IR emitter, a range sensor and an ambient light sensor in a three-in-one ready-to-use reflowable package, the VL6180 is easy to integrate and saves the end-product makers the long and costly optical and mechanical design optimizations. <a href="https://cdn.sparkfun.com/datasheets/Sensors/Proximity/DM00112632.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/12784">SparkFun ToF Range Finder Breakout - VL6180</a> (SEN-12784)</li><li><a href="https://www.sparkfun.com/products/12785">SparkFun ToF Range Finder Sensor - VL6180</a> (SEN-12785)</li></ul>
K PROD_ID:IC-12007
$ENDCMP
#
#End Doc Library
