(module LTR-301 (layer F.Cu) (tedit 200000)
  (descr "LTR-301 IR PHOTOTRANSISTOR (SIDE-RECEIVING)")
  (tags "LTR-301 IR PHOTOTRANSISTOR (SIDE-RECEIVING)")
  (attr virtual)
  (fp_text reference >NAME (at -2.667 0 90) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 2.794 0 90) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_line (start -2.159 -0.762) (end 2.159 -0.762) (layer F.SilkS) (width 0.127))
  (fp_line (start 2.159 -0.762) (end 2.159 0.762) (layer F.SilkS) (width 0.127))
  (fp_line (start 2.159 0.762) (end 0.762 0.762) (layer F.SilkS) (width 0.127))
  (fp_line (start 0.762 0.762) (end -0.762 0.762) (layer F.SilkS) (width 0.127))
  (fp_line (start -0.762 0.762) (end -2.159 0.762) (layer F.SilkS) (width 0.127))
  (fp_line (start -2.159 0.762) (end -2.159 -0.762) (layer F.SilkS) (width 0.127))
  (fp_line (start 0 -0.254) (end -0.381 0) (layer F.SilkS) (width 0.127))
  (fp_line (start 0 0.254) (end -0.381 0) (layer F.SilkS) (width 0.127))
  (fp_line (start -0.381 0) (end 0.381 0) (layer F.SilkS) (width 0.127))
  (fp_arc (start 0 0.762) (end 0.762 0.762) (angle 180) (layer F.SilkS) (width 0.127))
  (pad C thru_hole circle (at 1.27 0) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad E thru_hole circle (at -1.27 0) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
