(module TO220V (layer F.Cu) (tedit 200000)
  (descr "TO 220 VERTICAL PACKAGE WORKS WITH VARIOUS PARTS INCLUDING N-CHANNEL MOSFET SPARKFUN SKU: COM-10213")
  (tags "TO 220 VERTICAL PACKAGE WORKS WITH VARIOUS PARTS INCLUDING N-CHANNEL MOSFET SPARKFUN SKU: COM-10213")
  (attr virtual)
  (fp_text reference >NAME (at -5.842 -1.27 90) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 5.842 -1.016 90) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_line (start -5.08 -2.032) (end 5.08 -2.032) (layer F.SilkS) (width 0.06604))
  (fp_line (start 5.08 -2.032) (end 5.08 -3.048) (layer F.SilkS) (width 0.06604))
  (fp_line (start -5.08 -3.048) (end 5.08 -3.048) (layer F.SilkS) (width 0.06604))
  (fp_line (start -5.08 -2.032) (end -5.08 -3.048) (layer F.SilkS) (width 0.06604))
  (fp_line (start -5.08 -2.032) (end -5.08 0.381) (layer F.SilkS) (width 0.2032))
  (fp_line (start 5.08 -2.032) (end 5.08 0.381) (layer F.SilkS) (width 0.2032))
  (fp_line (start 5.08 -2.032) (end -5.08 -2.032) (layer F.SilkS) (width 0.2032))
  (fp_line (start -5.08 -2.032) (end -5.08 -3.048) (layer F.SilkS) (width 0.2032))
  (fp_line (start -5.08 -3.048) (end 5.08 -3.048) (layer F.SilkS) (width 0.2032))
  (fp_line (start 5.08 -3.048) (end 5.08 -2.032) (layer F.SilkS) (width 0.2032))
  (fp_line (start -4.191 1.27) (end -3.81 1.27) (layer F.SilkS) (width 0.2032))
  (fp_line (start 4.191 1.27) (end 3.81 1.27) (layer F.SilkS) (width 0.2032))
  (fp_arc (start -4.21132 0.40132) (end -4.191 1.27) (angle 92.7) (layer F.SilkS) (width 0.2032))
  (fp_arc (start 4.21132 0.40132) (end 5.08 0.381) (angle 92.7) (layer F.SilkS) (width 0.2032))
  (pad 1 thru_hole oval (at -2.54 0 180) (size 1.524 3.048) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 2 thru_hole oval (at 0 0 180) (size 1.524 3.048) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 3 thru_hole oval (at 2.54 0 180) (size 1.524 3.048) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
