(module MOLEX-1X4 (layer F.Cu) (tedit 200000)
  (descr "MOLEX 4-PIN PLATED THROUGH-HOLE")
  (tags "MOLEX 4-PIN PLATED THROUGH-HOLE")
  (attr virtual)
  (fp_text reference >NAME (at 0 -3.556) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 0 3.175) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_line (start -1.27 -3.048) (end -1.27 2.54) (layer F.SilkS) (width 0.127))
  (fp_line (start 8.89 -3.048) (end 8.89 2.54) (layer F.SilkS) (width 0.127))
  (fp_line (start 8.89 -3.048) (end -1.27 -3.048) (layer F.SilkS) (width 0.127))
  (fp_line (start 8.89 2.54) (end 7.62 2.54) (layer F.SilkS) (width 0.127))
  (fp_line (start 7.62 2.54) (end 0 2.54) (layer F.SilkS) (width 0.127))
  (fp_line (start 0 2.54) (end -1.27 2.54) (layer F.SilkS) (width 0.127))
  (fp_line (start 0 2.54) (end 0 1.27) (layer F.SilkS) (width 0.127))
  (fp_line (start 0 1.27) (end 7.62 1.27) (layer F.SilkS) (width 0.127))
  (fp_line (start 7.62 1.27) (end 7.62 2.54) (layer F.SilkS) (width 0.127))
  (pad 1 thru_hole rect (at 0 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 2 thru_hole circle (at 2.54 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 3 thru_hole circle (at 5.08 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 4 thru_hole circle (at 7.62 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
