(module 1X02_LOCK_LONGPADS (layer F.Cu) (tedit 5963D128)
  (descr "PLATED THROUGH HOLE - LONG PADS WITH LOCKING FOOTPRINT")
  (tags "PLATED THROUGH HOLE - LONG PADS WITH LOCKING FOOTPRINT")
  (attr virtual)
  (fp_text reference >NAME (at 0 -2.159) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 0 2.159) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_line (start 1.651 0) (end 0.889 0) (layer F.SilkS) (width 0.2032))
  (fp_line (start -1.27 0) (end -1.016 0) (layer F.SilkS) (width 0.2032))
  (fp_line (start -1.27 0) (end -1.27 -0.9906) (layer F.SilkS) (width 0.2032))
  (fp_line (start -1.27 -0.9906) (end -0.9906 -1.27) (layer F.SilkS) (width 0.2032))
  (fp_line (start -1.27 0) (end -1.27 0.9906) (layer F.SilkS) (width 0.2032))
  (fp_line (start -1.27 0.9906) (end -0.9906 1.27) (layer F.SilkS) (width 0.2032))
  (fp_line (start 3.81 0) (end 3.556 0) (layer F.SilkS) (width 0.2032))
  (fp_line (start 3.81 0) (end 3.81 0.9906) (layer F.SilkS) (width 0.2032))
  (fp_line (start 3.81 0.9906) (end 3.5306 1.27) (layer F.SilkS) (width 0.2032))
  (fp_line (start 3.81 0) (end 3.81 -0.9906) (layer F.SilkS) (width 0.2032))
  (fp_line (start 3.81 -0.9906) (end 3.5306 -1.27) (layer F.SilkS) (width 0.2032))
  (pad 1 thru_hole oval (at -0.127 0 180) (size 1.524 3.048) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 2 thru_hole oval (at 2.667 0 180) (size 1.524 3.048) (drill 1.016) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
