(module USB-A-S-NOSILK-FEMALE (layer F.Cu) (tedit 200000)
  (descr "USB TYPE 'A' FEMALE CONNECTOR - SMT NO SILK")
  (tags "USB TYPE 'A' FEMALE CONNECTOR - SMT NO SILK")
  (attr smd)
  (fp_text reference >NAME (at 8.89 -6.35) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 8.89 6.35) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_line (start 6.2357 -6.5659) (end -7.747 -6.5659) (layer Dwgs.User) (width 0.127))
  (fp_line (start 6.2357 6.5659) (end -7.747 6.5659) (layer Dwgs.User) (width 0.127))
  (fp_line (start -7.747 -6.477) (end -7.747 6.477) (layer Dwgs.User) (width 0.127))
  (fp_line (start 6.2484 -6.5024) (end 6.2484 6.5024) (layer Dwgs.User) (width 0.127))
  (fp_line (start 0 5.08) (end -6.35 4.445) (layer Dwgs.User) (width 0.127))
  (fp_line (start -6.35 4.445) (end -6.35 1.27) (layer Dwgs.User) (width 0.127))
  (fp_line (start -6.35 1.27) (end 0 0.635) (layer Dwgs.User) (width 0.127))
  (fp_line (start 0 -5.08) (end -6.35 -4.445) (layer Dwgs.User) (width 0.127))
  (fp_line (start -6.35 -4.445) (end -6.35 -1.27) (layer Dwgs.User) (width 0.127))
  (fp_line (start -6.35 -1.27) (end 0 -0.635) (layer Dwgs.User) (width 0.127))
  (pad D+ smd rect (at 6.75132 0.99822) (size 2.99974 0.89916) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad D- smd rect (at 6.75132 -0.99822) (size 2.99974 0.89916) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad GND smd rect (at 6.75132 3.49758) (size 2.99974 0.89916) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
  (pad SHLD thru_hole circle (at 2.54 6.5659) (size 3.3274 3.3274) (drill 2.3114) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad SHLD thru_hole circle (at 2.54 -6.5659) (size 3.3274 3.3274) (drill 2.3114) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad VBUS smd circle (at 6.75132 -3.49758) (size 2.99974 0.89916) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.1016))
)
