EESchema-DOCLIB  Version 2.0
#
$CMP AT25SF041
D AT25SF041 4Mb Serial Flash Memory 104MHz, SPI, 8-SOIC<li><a href= http://www.adestotech.com/wp-content/uploads/DS-AT25SF041_044.pdf >Datasheet</a></li> <b>SparkFun Products:</b><ul><li><a href= https://www.sparkfun.com/products/13231 >SparkFun ESP8266 Thing</a></li><li><a href= https://www.sparkfun.com/products/13711 >SparkFun ESP8266 Thing - Dev Board</a></li></ul> 
K PROD_ID:IC-12455
$ENDCMP
#
$CMP EEPROM-I2CEIAJ
D I2C EEPROMs, 24LC256 and others 24LC256 Series 256 kb I2C 2 Wire (32 k x 8 Bit) 2.5 V Serial EEPROM SMD - SOIC-8 <a href="">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/11703">SparkFun UDB5 - PIC UAV Development Board</a> (GPS-11703)</li></ul>
K PROD_ID:NA-XXXXX
$ENDCMP
#
$CMP EEPROM-I2CSMD
D I2C EEPROMs, 24LC256 and others 24LC256 Series 256 kb I2C 2 Wire (32 k x 8 Bit) 2.5 V Serial EEPROM SMD - SOIC-8 <a href="">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/11703">SparkFun UDB5 - PIC UAV Development Board</a> (GPS-11703)</li></ul>
K PROD_ID:IC-09714
$ENDCMP
#
$CMP SPI_FLASH-X25XXSMD
D 32M Serial Flash Memory 8pin SPI Flash series x25xx. Works with devices like W25X32 and BR25L32 <li><a href="http://www.macronix.com/Lists/Datasheet/Attachments/5031/MX25L3206E,%203V,%2032Mb,%20v1.5.pdf">Datasheet</a></li> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/10920">SparkFun Venus GPS Logger</a> (GPS-10920)</li></ul>
K PROD_ID:N/A
$ENDCMP
#
$CMP SPI_FLASH-X25XXSMD1
D 32M Serial Flash Memory 8pin SPI Flash series x25xx. Works with devices like W25X32 and BR25L32 <li><a href="http://www.macronix.com/Lists/Datasheet/Attachments/5031/MX25L3206E,%203V,%2032Mb,%20v1.5.pdf">Datasheet</a></li> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/10920">SparkFun Venus GPS Logger</a> (GPS-10920)</li></ul>
K PROD_ID:IC-09109
$ENDCMP
#
$CMP W25Q32FVSS
D W25Q32FV 32Mb (4MB) Serial Flash Memory The W25Q32FV support the standard Serial Peripheral Interface (SPI), Dual/Quad I/O SPI as  well as 2-clocks instruction cycle Quad Peripheral Interface (QPI). 104MHz, SPI, 8-SOIC-EIAJ <a href="http://www.winbond.com/resource-files/w25q32fv%20revh%20091613.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/13794">SparkFun Blynk Board - ESP8266</a> (WRL-13794)</li></ul>
K PROD_ID:IC-13229
$ENDCMP
#
$CMP W25Q32FVZP
D W25Q32FV 32Mb (4MB) Serial Flash Memory The W25Q32FV support the standard Serial Peripheral Interface (SPI), Dual/Quad I/O SPI as  well as 2-clocks instruction cycle Quad Peripheral Interface (QPI). 104MHz, SPI, 8-SOIC-EIAJ <a href="http://www.winbond.com/resource-files/w25q32fv%20revh%20091613.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/13794">SparkFun Blynk Board - ESP8266</a> (WRL-13794)</li></ul>
K PROD_ID:NA-XXXXX
$ENDCMP
#
#End Doc Library
