EESchema-DOCLIB  Version 2.0
#
$CMP ADS1015
D ADS1015 12-BIT ADC 12-Bit Del-Sig ADC<br>Four single-ended inputs or two differential inputs<br>Internal PGA<br>I<sup>2</sup>C interface<br>2.0-5.5V <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/13770">SparkFun Block for Intel Edison - ADC</a> (DEV-13770)</li></ul>
K PROD_ID:IC-12270
$ENDCMP
#
$CMP HX711
D AVIA Semiconductor HX711 - ADC 24-Bit Analog-to-Digital Converter for Weigh Scales<li><a href= https://cdn.sparkfun.com/datasheets/Sensors/ForceFlex/hx711_english.pdf >Datasheet</a></li> <b>SparkFun Products:</b><ul><li><a href= https://www.sparkfun.com/products/13879 >SparkFun Load Cell Amplifier - HX711 </a></li></ul> 
K PROD_ID:IC-12445
$ENDCMP
#
$CMP MAX31855K
D Cold-Junction-Compensated K-Thermocoupleto-DigitalConverter (-270 C to +1800 C) The MAX31855K performs cold-junction compensationand digitizes the signal from a type-K thermocouple.<br>The data is output in a 14-bit resolution, SPI -compatible,read-only format.<br>This converter resolves temperatures to 0.25 C, allows readings as high as +1800 C and as low as -270 C, and exhibits thermocouple accuracy of  2 C for temperatures ranging from -200 C to +700 C for K-type thermocouples. <a href="https://cdn.sparkfun.com/datasheets/Sensors/Temp/MAX31855K.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/13266">SparkFun Thermocouple Breakout - MAX31855K</a> (SEN-13266)</li></ul>
K PROD_ID:IC-12578
$ENDCMP
#
$CMP MCP4725SOT-23
D MCP4725 DAC Microchip 12-bit I2C DAC, SOT23-6 <a href="https://cdn.sparkfun.com/datasheets/BreakoutBoards/MCP4725_2009.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/12918">SparkFun I2C DAC Breakout - MCP4725</a> (BOB-12918)</li></ul>
K PROD_ID:IC-08886
$ENDCMP
#
$CMP PCM1803SMD
D PCM1803ADB STEREO ADC 24-bit <a href="">Datasheet</a> <h4>SparkFun Products</h4><ul><li>none</li></ul>stock = 62
K PROD_ID:IC-09251
$ENDCMP
#
$CMP VS1000
D VS1000D Ogg Vorbis Player IC with USB and NAND FLASH Interface 12 MHz LQFP-48   <a href="">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/8300">Storefront component: Ogg Vorbis Codec IC - VS1000D</a> (COM-08300)</li></ul>
K PROD_ID:LPA-12743 
$ENDCMP
#
$CMP VS1033_1053SMD
D VS1053B MP3 and MIDI Codec AAC/MP3/WMA/MIDI/Ogg Audio Player and Ogg Recording Device LQFP-48 7x7x1.4 mm <a href="http://www.sparkfun.com/datasheets/Components/SMD/vs1053.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/8892">Storefront component: MP3 and MIDI Codec - VS1053B</a> (COM-08892)</li><li><a href="https://www.sparkfun.com/products/12660">SparkFun MP3 Player Shield</a> (DEV-12660)</li><li><a href="https://www.sparkfun.com/products/11013">LilyPad MP3</a> (DEV-11013)</li><li><a href="https://www.sparkfun.com/products/10587">SparkFun Music Instrument Shield</a> (DEV-10587)</li></ul>
K PROD_ID:IC-12665
$ENDCMP
#
$CMP VS1063SMD
D MP3 and MIDI Codec - VS1063 AAC/MP3/WMA/MIDI/Ogg Audio Player and Ogg Recording Device LQFP-48 7x7x1.4 mm <a href="http://cdn.sparkfun.com/datasheets/Widgets/vs1063ds.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/11025">Storefront component:  MP3 and MIDI Codec - VS1063</a> (COM-11025)</li></ul>
K PROD_ID:IC-10870
$ENDCMP
#
$CMP WTV020SD
D WTV020SD Audio Module SD audio playback IC<br>Can play back .wav or .ad4 files from an SD card<br>SPI control or digital input trigger control<br>available in SSOP-20 or DIP-20 <a href="http://cdn.sparkfun.com/datasheets/Widgets/WTV020SD.pdf">Datasheet</a> <h4>SparkFun Products</h4><ul><li><a href="https://www.sparkfun.com/products/11125">SparkFun Audio-Sound Breakout - WTV020SD</a> (WIG-11125)</li></ul>
K PROD_ID:IC-11012
$ENDCMP
#
#End Doc Library
