(module PHOTOCELL (layer F.Cu) (tedit 200000)
  (descr "CDS PHOTOCOUNDUCTIVE PHOTOCELL (PTH)")
  (tags "CDS PHOTOCOUNDUCTIVE PHOTOCELL (PTH)")
  (attr virtual)
  (fp_text reference >NAME (at 0 -2.54) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_text value >VALUE (at 0 2.667) (layer F.SilkS)
    (effects (font (size 0.6096 0.6096) (thickness 0.127)))
  )
  (fp_line (start -0.99822 -1.99898) (end 0.99822 -1.99898) (layer F.SilkS) (width 0.2032))
  (fp_line (start 0.99822 1.99898) (end -0.99822 1.99898) (layer F.SilkS) (width 0.2032))
  (fp_arc (start -0.89916 -0.56388) (end -2.2987 -0.89916) (angle 72.5) (layer F.SilkS) (width 0.2032))
  (fp_arc (start 0.89916 0.56388) (end 2.2987 0.89916) (angle 72.5) (layer F.SilkS) (width 0.2032))
  (fp_arc (start 0.89916 -0.56388) (end 0.99822 -1.99898) (angle 72.5) (layer F.SilkS) (width 0.2032))
  (fp_arc (start -0.89916 0.56388) (end -0.99822 1.99898) (angle 72.5) (layer F.SilkS) (width 0.2032))
  (pad 1 thru_hole circle (at -1.99898 0) (size 1.6764 1.6764) (drill 0.79756) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
  (pad 2 thru_hole circle (at 1.99898 0) (size 1.6764 1.6764) (drill 0.79756) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1016))
)
